Windows XP

Introduction:
-------------
  This document shows you how to setup the driver and how to use the 
  enhanced functions by setting the custom keywords.

  Location of Driver:     \WINXP\DLKRTS.SYS

Installation:
-------------
  Before starting with the installation process, make sure that the 
  adapter is properly installed and configured.

   1.You will see there is an item:
     
        "D-Link DFE-538TX 10/100 Adapter"

     in the 'Network adapters' list in the Device Manager.

     The Device Manager can be invoked by choosing Start\Control Panel\
     System\Hardware (Tag)\Device Manager (button)

     We recommend you to install the updated driver from the distributing 
     disk by performing step 3 ~ 13.

   2.If Windows XP has not built the driver for DFE-538TX, obey
     step 5 ~ 13 to install the driver.

   3.Invoke the Device Manager. Right click the item

         "D-Link DFE-538TX 10/100 Adapter"

     in the 'Network adapters' list, and choose Properties.
     There will prompt the D-Link DFE-538TX 10/100 Adapter
     Properties window.

   4.Click the Driver tag, and choose the 'Update Driver' button.
     There wll prompt a Hardware Update Wizard window.
     Click 'Next'.

   5.The Wizard will ask you
     What do you want the wizard to do?
     Please choose
     Install from a list or specific location(Advanced)
     Click 'Next'.
     
   6.There will prompt a 'Please choose your search and installation 
     options' window. 
     Please choose 'Don't Search. I will choose the driver to install'
     option. Click 'Next'.

   7.There will prompt a "Hardware Type." window.
     Please select the Network adapters hardware type,and then 
     click 'Next'.

   8.Click 'Have Disk'.
     In 'Install From Disk' window, type the following path in the 
     combo list:

            EX:
               E:\WINXP

     Click 'OK'.  

   9.There will show

            "D-Link DFE-538TX 10/100 Adapter"

     in the 'Network Adapter' field.
     Click 'Next'.

  10.There will show

            "D-Link DFE-538TX 10/100 Adapter"

     in 'Hardware Installation' window.
     Click 'Next'.

  11.Windows XP will copy the driver and system files for the network.
     If there prompts a " ...has not passed Windows Logo testing...", 
     please click 'Continue Anyway' to continue the installation.

  12.Click 'Finish' to close the wizard, and the updated driver will 
     work for DFE-538TX.

  13.You will see

        "D-Link DFE-538TX 10/100 Adapter"

     in the 'Network adapters' list, and restart the computer.
