   Windows 2000

   Introduction:
   -------------
   This document describes the procedure to install  Windows 2000 driver 
   for D-Link DFE-538TX 10/100 Adapter.

   Location of Driver:     \WIN2000\DLKRTS.SYS

   Installing driver procedure on Microsoft Windows 2000:
   ------------------------------------------------------
   Before starting with the installation process, make sure that the 
   adapter is properly installed and configured.

   1.You will see there is an item:
     
        "D-Link DFE-538TX 10/100 Adapter"

     in the 'Network adapters' list in the Device Manager.

     The Device Manager can be invoked by choosing Start\Control Panel\System
     \Hardware (Tag)\Device Manager (button)

     We recommend you to install the updated driver from the distributing disk
     by performing step 3 ~ 11.

   2.If Windows 2000 has not built the driver for DFE-538TX, obey
     step 5 ~ 11 to install the driver.

   3.Invoke the Device Manager. Right click the item

         "D-Link DFE-538TX 10/100 Adapter"

     in the 'Network adapters' list, and choose Properties.
     There will prompt the D-Link DFE-538TX 10/100 Adapter
     Properties window.

   4.Click the Driver tag, and choose the 'Update Driver' button.
     There wll prompt a Upgrade Device Driver Wizard window.
     Click 'Next'.

   5.The Wizard will ask you
     What do you want the wizard to do?
     Please choose
       Display a list of the known drivers for this device so that I can 
       choose a specific driver.
     Click 'Next', it will prompt a 'Select Network Adapter' window.

   6.Click 'Have Disk'.
     In 'Install From Disk' window, type the following path in the combo 
     list:
            EX:
               E:\Win2000

     Click 'OK'.

   7.There will show

            "D-Link DFE-538TX 10/100 Adapter"

     in the 'Network Adapter' field.
     Click 'Next'.

   8.There will show

            "D-Link DFE-538TX 10/100 Adapter"

     in 'Start Device Driver Installation' window.
     Click 'Next'.

   9.Windows 2000 will copy the driver and system files for the network.
     If there prompts a Digital Signature Not Found window, please click 
     'Yes' to continue the installation.

  10.Finish the 'Update Driver', and the updated driver will work for
     DFE-538TX.

  11.You will see

        "D-Link DFE-538TX 10/100 Adapter"

     in the 'Network adapters' list.

Change the property of DFE-538TX:
---------------------------------
    There are some properties that you can change for your application.

    1. Connection Type: 100M Full Mode
                        100M Half Mode
                        10M Full Mode
                        10M Half Mode
                        Auto Mode       (Default value)

       You can change the speed to be 10M or 100M and change to be the Full
       duplex or Half duplex.
       The default value is Auto Mode,i.e. DFE-538TX will talk with connection
       Hub or Switch with auto-negotiation to decide the optimal connection
       type.
