
           D-Link DFE-550TX FAST Ethernet 10/100 Adapter Installation
                    for Windows 95 (retail) & Windows 95 OSR2

 Getting Started
 ---------------

    The Windows 95 installation diskettes or CD are required to complete
    the installation.

    Windows 95 (retail) Intallation Procedure
    -----------------------------------------

     1. Make sure your computer is power-off.

     2. Plug the adapter into one PCI slot of your computer.

     3. Turn on the power. Your computer should be booting.

     4. In the "New Hardware Found" window, choose
        "Driver from disk provided by hardware manufacturer" item.
        Then click "OK".

     5. Insert the driver diskette into the floppy disk drive.

     6. In the "Install From Disk" window, specify the path of the driver.

        Example:
                    A:\        (A: is floppy drive)
                OR
                    D:\        (D: is CD drive)

        Then click "OK".

     7. After finishing file copying, the Windows system will ask you
        to restart the system. Select "YES" to reboot.

    Windows 95 OSR2 Intallation Procedure
    -------------------------------------

     1. Make sure your computer is power-off.

     2. Plug the adapter into one PCI slot of your computer.

     3. Turn on the power. Your computer should be booting.

     4. Windows 95 will find new hardware, and
        "Update Device Driver Wizard" will appear.

     5. Insert the driver diskette into the floppy disk drive, and
        press "Next" to continue.

     6. The "Update Device Driver Wizard" should found the driver now,
        press "Finish" to continue. If wizard did not found the driver,
        press "Other Location" and specify the location of the driver.
        (ex. A:\OSR2, assume A: is floppy drive,
             D:\OSR2, asume D: is CD drive).

     7. After finishing file copying, the Windows system will ask you
        to restart the system. Select "YES" to reboot.


 Trouble Shooting
 ----------------
     - Everything is OK in Device Manager, but network adapter still
       does't function properly. Please make sure that your Computer
       name is different from others in the same network.  You can change
       your Computer name in

       "My Computer" -> "Control Panel" -> "Network" -> "Identification"
       icons

     - Everything appears to be OK but network adapter still doesn't
       function properly. Please make sure that the adapter is properly
       connected to a network device (ex: HUB) and the "connection type"
       for this adapter is set to "AutoSense" or the correct media type.
       You can check it in

       "My Computer" -> "Control Panel" -> "Network" -> "Properties"
       icons. Select "Advanced" item.


 Driver keywords
 ---------------

     - Open "My Computer" -> "Control Pannel" -> "Network" ->
       Double click "D-Link DFE-550TX ...", Select "Advanced" item.

       Connection Type      Specify the connection type for the adapter.
                            Default: AutoSense

       Network Address      You can set the Ethernet address for your
                            adapter. It is not recommended to use this
                            keyword. As you know two or more adapter in
                            the same network with same Ethernet address
                            will cause a little problem.

                            When using this keyword you need to input
                            exactly 6 bytes of Ethernet address using
                            one of the following format:

                              xx-xx-xx-xx-xx-xx
                            OR
                              xxxxxxxxxxxx

                            Default: read address from adapter ROM.

       802.1Q/1P VLAN       You can enable it for VLAN group.
       tagging              Default: disable

       VLAN ID              This value will active after 802.1Q/1P VLAN
                            tagging enable.

       GVRP		    Support GVRP and will active after 802.1Q/1P
                            VLAN tagging enable.
                            Default: disable
