
         D-Link DFE-550TX FAST Ethernet 10/100 Adapter Installation
                            for Windows 98, Windows 98 SE

 Getting Started
 ---------------

    The Windows 98 or Windows 98 SE installation CD are need to complete this
    install.

    Windows 98 Installation Procedure
    ---------------------------------
    Windows 98
    ----------    
     1. Make sure your computer is power-off.

     2. Plug the adapter into one PCI slot of your computer.

     3. Turn on the power. Your computer should be booting.

     4. Windows 98 will find new hardware, and
        "Add New Hardware Wizard" will appear.

     5. Insert the driver diskette into the floppy disk, and
        press "Next", and "Next" again in the following window.

     6.	Please check "Specify a location" and specify the path. 
        (A:\win98, assume A: is floppy drive),
        (D:\win98, assume D: is CD drive).

     7. The wizard should found the driver now. Follow the direction
        to complete installation.

     8. After finishing the installation, the Windows system will ask
        you to restart the system. Select "YES" to reboot.


    Windows 98 SE
    -------------    
     1. Make sure your computer is power-off.

     2. Plug the adapter into one PCI slot of your computer.

     3. Turn on the power. Your computer should be booting.

     4. Windows 98 will find new hardware, and
        "Add New Hardware Wizard" will appear.

     5. Insert the driver diskette into the floppy disk, and
        press "Next", and "Next" again in the following window.

     6.	Please check "Specify a location" and specify the path. 
        (A:\win98se, assume A: is floppy drive),
        (D:\win98se, assume D: is CD drive).

     7. The wizard should found the driver now. Follow the direction
        to complete installation.

     8. After finishing the installation, the Windows system will ask
        you to restart the system. Select "YES" to reboot.


 Trouble Shooting
 ----------------

     - Everything is OK in Device Manager, but network adapter still
       does't function properly. Please make sure that your Computer
       name is different from others in the same network.  You can change
       your Computer name in

       "My Computer" -> "Control Panel" -> "Network" -> "Identification"
       icons

     - Everything appears to be OK but network adapter still doesn't
       function properly. Please make sure that the adapter is properly
       connected to a network device (ex: HUB) and the "connection type"
       for this adapter is set to "AutoSense" or the correct media type.
       You can check it in

       "My Computer" -> "Control Panel" -> "Network" -> "Properties"
       icons. Select "Advanced" item.


 Driver keywords
 ---------------
     - Open "My Computer" -> "Control Pannel" -> "Network" ->
       Double click "D-Link DFE-550TX ...", Select "Advanced" item.

       Connection Type      Specify the connection type for the adapter.
                            Default: AutoSense

       Network Address      You can set the Ethernet address for your
                            adapter. It is not recommended to use this
                            keyword. As you know two or more adapter in
                            the same network with same Ethernet address
                            will cause a little problem.

                            When using this keyword you need to input
                            exactly 6 bytes of Ethernet address using
                            one of the following format:

                              xx-xx-xx-xx-xx-xx
                            OR
                              xxxxxxxxxxxx

                            Default: read address from adapter ROM.

       802.1Q/1P VLAN       You can enable it for VLAN group.
       tagging              Default: disable

       VLAN ID              This value will active after 802.1Q/1P VLAN
                            tagging enable.

       GVRP		    Support GVRP and will active after 802.1Q/1P 
                            VLAN tagging enable.
                            Default: disable
	        
