
           D-Link DFE-550TX 10/100 Adapter Installation
                for SCO OpenServer V5.0 MDI Driver


 Getting Started
 ---------------

0. Login as root user. (On maintenance mode)

1. Using "custom" to install the driver

    1.1 Prepare an image file

        Copy d5X.IMG onto SCO OpenServer and rename it to VOL.000.000

            # mkdir /usr/test
            # doscp a:/<PATH>/d5X.IMG /usr/test/VOL.000.000
            OR
	    # cp /cd_dir/<PATH>/d5x.IMG /usr/test/VOL.000.000
			
	      * <PATH> is the driver directory.
	      * cd_dir is CD ROM driver that had been mounted.	
                Note: Please log in as root and mount the CD-ROM
                      using the following commands:
                      
	              # cd /
                      # mkdir cd_dir
                      # mount -r /dev/cd0 /cd_dir

    1.2 Execute "custom"

        /* A menu selection screen will be popped up */
        Using [->] key to move cursor to "Software" menu item then
        press [] key to get into pull down menu then move to
        "Install New..." then press [ENTER] key


          赏屯屯屯屯?Begin Installation on scoopen 屯屯屯屯屯?
          ?                                                  ?
          ? What host (machine) do you want to install from? ?
          ?                                                  ?
          ? 谀哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪目 ?
          ? ?*> From scoopen                              ??
          ? ? > From another host                         ??
          ? 滥哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪馁 ?
          ?                                                  ?
          耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪?
          篬 Continue ]        [ Cancel ]         [ Help]     ?
          韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯?

        Select From scoopen and use [TAB] key to move cursor to
        [ Continue ] then press [ENTER] key and press [] key to get
        into pull down menu

          赏屯屯屯屯屯屯屯屯屯屯屯?Select Media 屯屯屯屯屯屯屯屯屯屯屯屯?
          ?                                                             ?
          ? Insert media, and select media device.                      ?
          ?                                                             ?
          ?              谀哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪目 ?
          ? Media Device:硘Floppy Disk Driver 0_____________________|v??
          ?              郎屯屯屯屯屯屯屯屯屯屯屯屯荒哪哪哪哪哪哪哪哪馁 ?
          ?               黑哪哪哪哪哪哪哪哪哪哪哪亢                    ?
          ?               撼*Floppy Disk Driver 0 澈                    ?
          ?               撼 Media Images         澈                    ?
          耗哪哪哪哪哪哪哪暮滥哪哪哪哪哪哪哪哪哪哪馁耗哪哪哪哪哪哪哪哪哪暮
          篬 Continue ]    韧屯屯屯屯屯屯屯屯屯屯屯图          [  Help  ]?
          韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯图


        -> Select "Media Images" and use [TAB] key to move cursor to
           [ Continue ] then press [ENTER] key then press [ENTER] key
           again

 赏屯屯屯屯屯屯屯屯屯屯屯 Enter Image Directory 屯屯屯屯屯屯屯屯屯屯屯屯屯?
 ?                                                                       ?
 ?Enter the full path to the directory containing media images.          ?
 ?                                                                       ?
 ?Image Directory: |/usr/test__________________________________________| ?
 ?                                                                       ?
 ?Note: media images must follow the naming convention VOL.000.000, etc. ?
 ?                                                                       ?
 ?                                                                       ?
 ?                                                                       ?
 耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪暮
 篬   OK   ]                     [ Cancel ]                     [  Help  ]?
 韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯图

            -> Input the path name where VOL.000.000 is located as above
               path name is /usr/test


 赏屯屯屯屯屯屯屯屯屯屯屯 Install Preference on scoopen 屯屯屯屯屯屯屯屯屯屯?
 ?                                                                         ?
 ?Installing: D-Link DFE-550TX PCI Fast Ethernet Device Driver (version 1.0?
 ?                                                                         ?
 ?Do you want a FULL or PARTIAL installation?                              ?
 ?                                                                         ?
 耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪暮
 篬  Full   ]           [ Partial ]         [ Cancel  ]          [  Help   ]?
 韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯图

        Using [TAB] key to move cursor to [ Full ] then press [ENTER] key

        After the installation progress the following message is displayed


                       赏屯屯屯屯屯 Question 屯屯屯屯屯?
                       ?    Installation complete     ?
                       耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪?
                       ?           [ OK ]             ?
                       韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯?

        Press [Enter] key then you will find out that

                D-Link DFE-550TX PCI Fast Ethernet Device Driver (ver 1.0.1)

        is added to the package list

        Using [<-] key to move cursor back to "Host" menu item then
        press [] key to get into pull down menu then move to "Exit"
        then press [ENTER] key

        Now that the driver is installed in the system successfully.


2. Using "netconfig" to configure the driver

   /* A menu selection screen will be popped up */
   At "Hardware" menu item press [] key to get into pull down menu then
   move to "Add new LAN adapter" then press [ENTER] key

   If you got a PCI NIC inserted on your machine, it will list as
   following:


赏屯屯屯屯屯屯屯屯屯屯屯屯屯 Add new LAN adapter 屯屯屯屯屯屯屯屯屯屯屯屯屯屯?
篢he following adapters have been found:                                     ?
黑哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪亢
撼*   D-Link DFE-550TX 10/100 Adapter SCO5 driver - PCI Bus# 0, PCI Device  澈
撼                                                                          澈
撼                                                                          澈
撼                                                                          澈
撼                                                                          澈
豪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪俸
篬 Configure hardware not listed above... ]                                  ?
耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪暮
篬 Continue ]                       [  Cancel  ]                   [  Help  ]?
韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯图

       If the "D-Link DFE-550TX 10/100 Adapter SCO5 driver" has been
       displayed press [ENTER] directly, otherwise using [TAB] key to
       move to "Configure hardware not listed above..." then press
       [ENTER] key


赏屯屯屯屯屯屯屯屯屯屯屯屯屯 Add new LAN adapter 屯屯屯屯屯屯屯屯屯屯屯屯屯屯?
篠elect network adapter to be added:                                         ?
黑哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪亢
撼*   3Com EtherLink 16/16TP Adapter                                        ^?
撼                   .                                                      *?
撼                   .                                                      *?
撼                   .                                                      *?
撼                   .                                                      *?
撼                   .                                                      *?
撼                   .                                                      *?
撼                   .                                                      *?
撼    D-Link DFE-550TX 10/100 Adapter SCO5 driver                           *?
撼                   .                                                      澈
撼                   .                                                      澈
撼                   .                                                      澈
撼                   .                                                      澈
撼                   .                                                      澈
撼                   .                                                      v?
豪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪俸
耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪暮
篬 Continue ]                       [  Cancel  ]                   [  Help  ]?
韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯图

   Using [] key to move to "D-Link DFE-550TX 10/100 Adapter SCO5 driver"
   then press [ENTER] key.

  赏屯屯屯屯屯屯屯屯屯屯 Network Driver Configuration 屯屯屯屯屯屯屯屯屯屯?
  ?                                                                      ?
  篍nter the configuration of D-Link DFE-550TX 10/100 Adapter SCO5 driver:?
  ?                                                                      ?
  ?               谀哪哪哪哪哪哪哪哪哪哪哪哪哪目 [ Advanced   ]          ?
  ?    PCI Bus#:  硘 0_______________________|v?  Options...            ?
  ?               滥哪哪哪哪哪哪哪哪哪哪哪哪哪馁                         ?
  ?               谀哪哪哪哪哪哪哪哪哪哪哪哪哪目                         ?
  ? PCI Device#:  硘 0_______________________|v?                        ?
  ?               郎屯屯屯屯荒哪哪哪哪哪哪哪哪馁                         ?
  ?               诤谀哪哪目耗哪哪哪哪哪哪哪哪目                         ?
  篜CI Function#:  澈? 9   ^篲_______________|v?                        ?
  ?               篮? 10  澈哪哪哪哪哪哪哪哪哪?                        ?
  ?                撼  11  *?                                           ?
  ?  * - indicates 撼  12  澈ith other hardware                          ?
  耗哪哪哪哪哪哪哪哪撼* 13  澈哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪?
  篬   OK   ]       撼  14  v?   [ Cancel ]                   [  Help  ] ?
  韧屯屯屯屯屯屯屯屯豪哪哪哪俸屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯?
                    韧屯屯屯图

   The above screen let you fill the information of where your PCI adapter
   is located by specifying PCI Bus#, PCI Device# and PCI Function#.

   Note1: If you can not make sure the PCI parameters or your PCI Device#
          can not be found in the list, just leave them as default values,
          continue the following installation, after the driver is
          installed and system is re-linked, reboot the system then driver
          will search PCI Ethernet card automatically.

   "Advanced Options" let you specify what media type is connectted.
   If you select it the following screen will be popped up

 赏屯屯屯屯屯屯屯屯?Advanced Network Driver Configuration 屯屯屯屯屯屯屯?
 ?                                                                      ?
 篍nter the configuration of D-Link DFE-550TX 10/100 Adapter SCO5 driver:?
 ?                                                                      ?
 ?                  谀哪哪哪哪哪哪哪哪哪哪哪哪?                        ?
 篗edia/Cable Type:  硘 AUTOSENSE____________|v?                        ?
 ?                  郎屯屯屯屯屯屯屯屯屯荒哪哪?                        ?
 ?                   ?谀哪哪哪哪哪哪哪亢                               ?
 ?  * - indicates con?? AUTOSENSE    澈 hardware                      ?
 耗哪哪哪哪哪哪哪哪哪暮 ? TP           澈哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪暮
 篬   OK   ]          ?? TP_FD        澈cel ]                [  Help  ]?
 韧屯屯屯屯屯屯屯屯屯秃 ? TX100        澈屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯图
                      ?? TX100_FD     澈
                      ?滥哪哪哪哪哪哪哪俸
                      韧屯屯屯屯屯屯屯屯图

   Select the connective media then press [ENTER] key to go back to
   "Network Driver Configuration" screen.

   Using [TAB] key to move cursor to "OK" then press [ENTER] key.

   赏屯屯屯屯屯屯屯屯屯屯屯屯?Information 屯屯屯屯屯屯屯屯屯屯屯屯屯屯?
   ?--  Please verify adapter is set to the configuration just entered?
   耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪?
   ?                             [ OK ]                               ?
   韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯?

   Press [ENTER] key.


赏屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯?Add Protocol 屯屯屯屯屯屯屯屯屯屯屯屯屯屯?
篠elect one networking product to be added to                                ?
篋-Link DFE-550TX 10/100 Adapter SCO5 driver:                                ?
黑哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪亢
撼 HW D-Link DFE-550TX 10/100 Adapter SCO5 driver                           澈
撼*   - SCO IPX/SPX                                                         澈
撼    - SCO TCP/IP                                                          澈
撼                                                                          澈
撼                                                                          澈
豪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪俸
耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪暮
篬  Add   ]                        [ Cancel ]                      [  Help  ]?
韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯图

   Using [] key to move cursor to "SCO TCP/IP" then press [ENTER] key.

   赏屯屯屯屯屯屯屯 SCO TCP/IP Configuration 屯屯屯屯屯屯屯屯?
   ?                                                        ?
   ?                                                        ?
   ?                                                        ?
   ? Local Host Name:  |scoopen_____________| [ Advanced   ]?
   ?      IP Address:  |192.9.200.1_________|   Options...  ?
   ?         Netmask:  |255.255.255.0_______|               ?
   築roadcast Address:  |192.9.200.255_______|               ?
   ?     Domain Name:  |scoopen.com_________|               ?
   ? TCP connections:  |256_________________|               ?
   ?     Pseudo ttys:  |32__________________|               ?
   ?                                                        ?
   ?                                                        ?
   耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪?
   ?[   OK   ]             [ Cancel ]            [  Help   ]?
   韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯?

   Input the required information then use [TAB] key to move cursor to
   "OK" then press [ENTER] key.

赏屯屯屯屯屯屯屯屯屯屯屯屯屯屯 Message 屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯突
?The following products were successfully configured into the system   ?
?SCO TCP/IP                                                            ?
?D-Link DFE-550TX 10/100 Adapter SCO5 driver - PCI Bus# 0,PCI Device# 1?
?                                                                      ?
耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪?
篬 OK ]                                                       [ Help ]  ?
韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯?

   Press [ENTER] key


   At "Hardware" menu item press [] key to get into pull down menu then
   move to "Exit" then press [ENTER] key

  赏屯屯屯屯屯屯屯屯屯屯屯 Question 屯屯屯屯屯屯屯屯屯屯屯屯?
  ?    The Unix kernel must be re-linked before the changes?
  ???  made here will have an effect.                      ?
  ?    Do you want to re-link the kernel now?              ?
  耗哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪哪?
  ?[ Yes ]                                          [ No ] ?
  韧屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯屯?

   Press [ENTER] key

   Do you want this kernel to boot by default (y/n)    y

   Do you want the kernel environment rebuilt (y/n)    y

3. Reboot unix

   # shutdown -y -g0

***************************************************
* Another way to specify driver's PCI parameters  *
***************************************************

. Another way to modify PCI parameters is at booting
   time, shown as below:

   1. Specify PCI Bus#, PCI Device# and PCI Function#

       Boot
       : unix net.mdi=d5X(0) net.param=(pcb:0,pcd:14,pcf:0)

   2. Auto-search PCI adapter card

       Boot
       : unix net.mdi=d5X(0)


Note2: The IRQ number must match with the value set in ROM-BIOS before you
       specify this value, please check it.
       The IRQ for PCI bus can be accessed by pressing [DEL] key when
       system is power on and choose the proper select item to set IRQ
       for PCI bus.

       Example: ROM PCI/ISA BIOS (2A4X5C31)
                   PCI/GREEN FUNCTION SETUP
                  AWARD SOFTWARE, INC.

             Press [DEL] key  -->  PCI/GREEN FUNCTION SETUP

                                   Slot 3 Using INT# : A-PIRQ1
                                           .
                                           .
                                           .
                                   PIRQ1# Connect IRQ: 5 By Single
                                                       ~


