
          D-Link DFE-550TX 10/100 Adapter Installation
                   for Lantastic


 Getting Started
 ---------------
    Lantastic 5.0 Install
    ---------------------
        Using NDIS driver
        -----------------
        - For NDIS driver support "DLH5X.DOS" driver for PCI
          Family Adapter. User can use "DLH5X.DOS" driver to replace
          AEXNDIS.DOS which is the NDIS driver offered by ARTISOFT.

                *** CONFIG.SYS ****
                DEVICE=C:\LANTASTI\PROTMAN.DOS /I:C:\LANTASTI
                --------------------------------------------------------
                DEVICE=C:\LANTASTI\AEXNDIS.DOS     -------> By Lantastic

                * please replace to *

                DEVICE=C:\LANTASTI\DLH5X.DOS     -------> By Vendor
                --------------------------------------------------------


                *** STARTNET.BAT ***
                --------------------------------------------------------
                C:\LANTASTI\AI-NDIS BIND_TO=AEXNDIS_NIF

                * please replace to *

                C:\LANTASTI\AI-NDIS BIND_TO=DLH5X_NIF
                --------------------------------------------------------
                C:\LANTASTI\AILANBIO
                C:\LANTASTI\REDIR MachineName


                *** PROTOCOL.INI ***
                --------------------------------------------------------
                [AEXNDIS_NIF]
                   DRIVERNAME = AEXNDIS$

                * please replace to *

                [DLH5X_NIF]
                   DRIVERNAME = DLH5X$
                --------------------------------------------------------

          Comments:
             If you are using PROTMAN.DOS V1.x, you must use the
             NO_BIND option on the AI-NDIS command line in the
             STARTNET.BAT, and you must run NETBIND.EXE V1.x before
             AILANBIO.EXE.


    Lantastic 6.0 Install
    ---------------------
        Using NDIS driver
        -----------------
        - To install NDIS driver "DLH5X.DOS", user can use Lantastic
          6.0 install program, and select "NDIS support for network
          adapters" then type path "C:\LANTASTI" (specify by install
          program).
          Install program will search "DLH5X.DOS" and "PROTOCOL.INI"
          and copy these two files to target directory.

        - If user already installed Lantastic 6.0 and want to install
          PCI Fast Ethernet Adapter, just replace AEXNDIS.DOS with NDIS
          driver "DLH5X.DOS" at CONFIG.SYS

          NOTE: "DLH5X.DOS" is an NDIS driver supported by Vendor.
                "AEXNDIS.DOS" is an NDIS driver supported by ARTISOFT

                *** CONFIG.SYS ***
                DEVICE=C:\LANTASTI\PROTMAN.DOS /I:C:\LANTASTI
                --------------------------------------------------------
                DEVICE=C:\LANTASTI\AEXNDIS.DOS  -------> By Lantastic

                * please replace to *

                DEVICE=C:\LANTASTI\DLH5X.DOS   -------> By Vendor
                --------------------------------------------------------


                *** STARTNET.BAT ***
                @echo ===== Begin Lantastic configuration =====
                SET LAN_CFG=C:\LANTASTI
                PATH C:\LANTASTI;%PATH%
                SET LAN_DIR=C:\LANTASTI.NET
                rem Please obtain the NETBEUI.EXE program from Microsoft
                NETBEUI
                --------------------------------------------------------
                AI-NDIS BIND_TO=AEXNDIS_NIF

                * please replace to *

                AI-NDIS BIND_TO=DLH5X_NIF
                --------------------------------------------------------
                AILANBIO @STARTNET.CFG
                REDIR  LANTA @STARTNET.CFG
                SERVER C:\LANTASTI.NET @STARTNET.CFG
                NET LOGIN \\LANTA
                @echo ===== End LANtastic configuration =====


                *** Protocol.ini ***
                [NETBEUI_XIF]
                    DriverName = netbeui$
                    Sessions = 6
                    NCBS = 12
                --------------------------------------------------------
                    Bindings = AEXNDIS_NIF

                * please replace to *

                    Bindings = DLH5X_NIF
                --------------------------------------------------------
                    LANABASE = 1
                --------------------------------------------------------
                [AEXNDIS_NIF]
                    DRIVERNAME = AEXNDIS$

                    * please replace to *

                [DLH5X_NIF]
                    DRIVERNAME = DLH5X$
                --------------------------------------------------------

        Using ODI DOS driver
        --------------------
        - ODI for DOS driver, support "DLH5X.COM" driver for PCI
          Family Adapter. User can use "DLH5X.COM" driver to replace
          NRODI.COM which is the ODI for DOS driver offered by ARTISOFT.

          Note: Because DLH5X.COM following HSM v4.0 spec, please save
                LSL.COM, IPXODI.COM that original supported by Lantastic.
                Copy both LSL.COM, IPXODI.COM from release driver diskette
                to target directory C:\LANTASTI.

                *** STARTNET.BAT ***
                @echo ===== Begin Lantastic configuration =====
                SET LAN_CFG=C:\LANTASTI
                PATH C:\LANTASTI;%PATH%
                SET LAN_DIR=C:\LANTASTI.NET
                SET NWDBPATH=C:\Lantasti\NW
                LSL     --> Please use new release driver
                NRODI   --> please replace to DLH5X
                ODINSUP
                IPXODI  --> Please use new release driver
                --------------------------------------------------------
                AI-NDIS BIND_TO=NRODI

                * please replace to *

                AI-NDIS BIND_TO=DLH5X
                --------------------------------------------------------
                AILANBIO @STARTNET.CFG
                REDIR  LANTA @STARTNET.CFG
                SERVER C:\LANTASTI.NET @STARTNET.CFG
                NET LOGIN \\LANTA
                @echo ===== End LANtastic configuration =====


                *** NET.CFG ***
                Please add below string into NET.CFG file.

                Link Driver DLH5X
                    Frame Ethernet_802.3