
            D-Link DFE-550TX FAST Ethernet 10/100 Adapter Installation
                              for Windows NT V4.0


 Getting Started
 ---------------

    - Start your Windows NT 4.0 PC normally and inserting the network
      adapter into your computer.

    - Open "My Computer" -> "Control Panel" -> "Networks" icons.

    - Select "Add adapter" -> "Have disk" items.
      Type the following (assume the driver is located at A:\)

            A:\winnt	(A: is floppy drive)
			OR 
            D:\winnt	(D: is CD drive)

      Select the "D-Link DFE-550TX ...".

    - Windows NT 4.0 will copy the driver files from the driver disk.
      It also will pop up the configuration window, you can assign the
      "Connection Type" and "Network Address" here.

    - After finishing file copy, Windows NT 4.0 will ask you to
      reboot the PC. Select YES.

    - Restart the computer.


 How to configure VLAN ID and GVRP
 ---------------------------------
    System requirement: Windows NT 4.0 + SP5 (or later).
    
    - Please install adpcfg.exe after driver install successfully. 
      The setup program will upadte new system files. You must restart the 
      system and continue the installation.
    - Select "D-Link Network Adapter" --> "D-Link Adapter Configuration" 
      on Start menu.
    - PLease select "VLAN" item and set the VLAN ID and GVRP.
    - The VLAN ID and GVRP will active after system restart.

  

    Driver keywords:
    ----------------

    - Open "My Computer" -> "Control Pannel" -> "Network" ->
      Double click "D-Link DFE-550TX ..."

      Connection Type   Specify the connection type for the adapter.
                        Default: AutoSense

      Network Address   You can set the Ethernet address for your adapter.
                        It is not recommended to use this keyword. Please
                        use default value if possible.
                        As you know two or more adapter in the same
                        network with same Ethernet address will cause
                        a little problem.

                        When using this keyword you need to input exactly
                        6 bytes of Ethernet address using one of the
                        following format:

                             xx-xx-xx-xx-xx-xx
                           OR
                             xxxxxxxxxxxx

                           Default: read address from adapter ROM.

       802.1Q/1P VLAN   You can enable it for VLAN group.
       tagging          Default: disable

       VLAN ID          This value will active after 802.1Q/1P VLAN
                        tagging enable.

       GVRP	        Support GVRP and will active after 802.1Q/1P
                        VLAN tagging enable.
                        Default: disable
