
                  D-Link DFE-550TX 10/100 Adapter Packet Drivers
                           Installation Overview


 User's Guide
 ------------

        File                  Description
    ------------    --------------------------------
    PCNFS.TXT       Sun PC-NFS installation document
    PCTCP.TXT       FTP PC/TCP installation document
    PDIPX.TXT       IPX SHELL installation document
    NCSA.TXT        NCSA installation document
    WINSOCK.TXT     Winsock installation document

    DEVICE = DLH5X.SYS [/option] <packet_int_no>
    DLH5X.COM [/option] <packet_int_no>

    Packet Driver Parameters:


        <packet_int_no> is the software interrupt vector number used by
                        the packet driver program, which can be from
                        96 to 128.

                        Note: <packet_int_no> can be hex or decimal
                              number.
                              hex - start with '0x'.
                                ex. >DLH5X 0x62
                              dec - start with nonzero digit.
                                ex. >DLH5X 98


        </d>            Delay Initial - The driver program will not
                        initialize the network interface card until the
                        packet driver program is accessed by its upper
                        layer program first time.

        </w>            the /w parameter is for use with the Windows
                        environment only.

        </u>            is to unload the driver program from memory.
                        The program will automatically search for Packet
                        driver to unload.

        </n>            NetWare conversion

     To select media type, you can use :

        </autosense>    this is the default setting. It let you able to
                        change media without restart the driver.

        </10baset>      Select Twisted Pair interface running in 10MBps
        				mode.

        </10basetfd>    Select Twisted Pair interface running in 10MBps
        				full duplex mode.

        </100basetx>    Select Twisted Pair interface running in 100MBps
        				mode.

        </100basetxfd>  Select Twisted Pair interface running in 100MBps
        				full duplex mode.

     To set descriptor number, you can use :

        </tx_buffers=>  Set tx buffer number.

        </rx_buffers=>  Set rx buffer number.


