
      D-Link DFE-570TX PCI Fast Ethernet Server Adapter Installation
                          for Windows NT V4.0


 Getting Started
 ---------------

    - Start your Windows NT 4.0 PC normally and inserting the network
      adapter into your computer.

    - Open "My Computer" -> "Control Panel" -> "Networks" icons.

    - Select "Add adapter" -> "Have disk" items.
      Type the following (assume the driver is located at A:\ or CD-ROM D:\)

            A:\ or D:\

      Select the "D-Link DFE-570TX PCI ..".

    - Windows NT 4.0 will copy the driver files from the driver disk.
      It also will pop up the configuration window, you can assign the
      "Connection Type" and "Network Address" here.

    - After finishing file copy, Windows NT 4.0 will ask you to
      reboot the PC. Select YES.

    - Restart the computer.


    Driver keywords:
    ----------------

    - Open "My Computer" -> "Control Pannel" -> "Network" ->
      Double click "D-Link DFE-570TX PCI .."

      Connection Type   Specify the connection type for the adapter.
                        Default: AutoSense

      Network Address   You can set the Ethernet address for your adapter.
                        It is not recommended to use this keyword. Please
                        use default value if possible.
                        As you know two or more adapter in the same
                        network with same Ethernet address will cause
                        a little problem.

                        When using this keyword you need to input exactly
                        6 bytes of Ethernet address using one of the
                        following format:

                             xx-xx-xx-xx-xx-xx
                           OR
                             xxxxxxxxxxxx

                           Default: read address from adapter ROM.
