
              D-Link DFE-570TX PCI Fast Ethernet Server Adapter

 Contents
 ========
    - Introduction
    - Revision History
    - Support Options
    - Copyrights, Trademarks

 Introduction
 ============
        
    The DFE-570TX Server Adapter will provide high performance solution and 
    safe the server PCI bus slot isn't enough problem. Each can provide 10M 
    or 100M half/full duplex connection to Switch. The ports running in 10M 
    or 100M wouldn't share one collision domain. These 4 ports can aggregate
    the throughput to 800Mbps at full-duplex mode. The built-in driver-level
    software can provide two feature for Sever connection- Fault-Tolerance 
    and Load-Balance. This software provides dynamic fail over and allows 
    customers to load balance network traffic across multiple network ports
    in this card.  It ensures that users maintain non-stop access to key 
    resources on the network, even if one or more of the network interface
    connections goes down. If a connection to an port is lost, this software
    will instantly take the fault-port out of the array and balance the 
    traffic across the remaining ports with no loss of data and, just as 
    importantly, without loss of connection. Also, when an adapter with 
    an NDIS 4.0 driver is brought back online, built-in software will 
    instantaneously add the adapter into the array and redistribute the 
    traffic.
    
    You can get latest releases of drivers from D-Link's Web site 
    (http://www.dlink.com). We hope our new readmes and installations
    will minimize the users effort to make our products work. Should there
    be further recommendations please contact the support manager at the
    local D-Link Office listed bellow.
    


 Revision History
 ================
     * CD-R Revision 20000601
      
      - Upgrade D-Link array software of NT4.0 from V1.1b to 2.03 
        (Provides detailed Throughput graphing and reporting)

      - Support D-Link array software (ver 2.1) for Windows 2000

      - Upgrade oemsetup.inf (v2.03) for NT4.0 SP6A.

     * Diskette Revision 990601     

      - Upgrade oemsetup.inf (v1.1b) for NT4.0 SP5.

     * Diskette Revision 990201     
      
      - Upgrade Fault-Tolerance and Load-Balance Software (V1.1a).
      - Upgrade MIB files .

     * Check http://www.dlink.com for any driver not in this diskette ,or
       any newest releases of drivers.

     * Diskette Revision 981201

      - Support Windows NT 4.0 Server Driver (V4.31.00).
      - Support Fault-Tolerance and Load-Balance Software (V1.1a). 

    
 Support Options
 ===============

    For technical support, you may contact your authorized D-Link
    distributor, dealer or the following D-Link branch offices.

    Australia       Web Site:  http:\\www.dlink.com.au
                    Tel: +61(2)9417-7100    Fax: +61(2)9417-1077
    
    Canada          Web Site:  http:\\www.dlink.ca
                    Tel: +1(905)829-5033    Fax: +1(905)829-5223 

    Chile           Web Site: http:\\www.dlink.cl
                    Tel: +56(2)232-3185     Fax: +56(2)232-0923 
 
    China           Web Site:  http:\\www.dlink.co.cn
                    Tel: +86(10)6846-7106~9 Fax: +86(10)6846-7110  

    Denmark         Web Site:  http:\\www.dlink.dk
                    Tel: +45(43)969-040     Fax: +45(43)424-347

    Egypt           Web Site:  http:\\www.dlink-me.com
                    Tel: +202-245-6176      Fax: +202-245-6192 

    France          Web Site:  http:\\www.dlink-france.fr 
                    Tel: +33(1)3023-8688    Fax: +33(1)3023-8689

    Germany         Web Site:  http:\\www.dlink.de
                    Tel: +49(6192)97110     Fax: +49(6192)9711-11

    India           Web Site:  http:\\www.dlink.india.com 
                    Tel: +91(22)652-6696    Fax: +91(22)652-8914

    Itlay           Web Site:  heep:\\www.dlink.it
                    Tel: +39(02)2900-0676   Fax: +39(02)2900-1723

    Japan           Web Site:  http:\\www.d-link.co.jp 
                    Tel: +81(3)5434-9678    Fax: +81(3)5434-9868

    Russia          Tel: +7(095)737-3389    Fax: +7(095)737-3390

    Singapore       Web Site:  http:\\www.dlink.intl.com
                    Tel: +65-774-6233       Fax: +65-774-6322

    S. Africa       Tel: +27(0)1266-52165   Fax: +27(0)1266-52186

    Sweden          Web Site:  http:\\www.dlink.se
                    Tel: +46(0)8564-61900   Fax: +46(0)8564-61901

    Taiwan          Web site:  http:\\www.dlinktw.com.tw
                    Tel: +886(2)910-2626    Fax: +886(2)910-1515

    U.K.            Web Site:  http:\\www.dlink.co.uk
                    Tel: +44(20)8235-5555   Fax: +44(20)8235-5500

    U.S.A.          Web Site:  http:\\www.dlink.com
                    Tel: +1(949)788-0805    Fax: +1(949)753-7033
                      
 
    The BBS communication setup information is as follows :

    Speed     :  2400-14400  baud                           - Germany
                 2400-9600   baud                           - Asia,Taiwan
                 14400-16800 baud                           - Canada
                 9600-14400  baud V32, V32bis, V42, V42bis  - U.S.A.
                 2400-19200  baud V24, V32, V32bis, V42bis  - U.K. & Europe
    Parity    : none
    Data bits : 8
    Stop bit  : 1

 Copyrights, Trademarks
 ======================
    All documents and software provided herewith are Copyright (c)2000
    D-Link Corporation. All rights reserved.

    Windows NT 4.0 is trade name of Microsoft Corporation.

    Other trademarks or trade names used herein are properties of the
    respective owners.
