
            D-Link DFE-580TX Quad Channel Server Card Installation
                            for Windows 2000

 Getting Started
 ---------------

    The Windows 2000 installation CD is needed to complete this
    installation.

    Windows 2000 Installation Procedure
    -----------------------------------

    Update driver from diskette/CD-ROM
    ----------------------------------
    The following steps can help you update the bundled driver to
    the one in the Adapter Drivers Diskette/CD-ROM.

     1. Open Control Panel, double click "System" icon to open System
        Properties.

     2. In the "Hardware" sheet, you can see the "Device Manager" bottum.
        Click to open Device Manager.

     3. Use the tool bar to make sure you "View" "Devices by type".
        Than you will able to find

        D-Link DL10050 based 10/100 Adapter

        in "Network Adapters" group. Double click it to open its property.

     4. In the "Driver" sheet of the adapter's properties, there is a button
        named "Update Driver". Click it, the Upgrade Device Driver Wizard
        will show up to help updating the driver.

     The following steps will lead you through the wizard ...

     1. The first page is the welcome messages, click "Next" to continue.

     2. Select "Search for a suitable driver for my device (recommanded)",
        and click "Next".

     3. Check "Specify a location" only. Click "Next" to continue.

     4. Specify the path.
        (A:\ , assume A: is floppy drive)
        (D:\ , assume D: is CD drive) 
        
     5. The wizard will find the specified driver.

        D-Link DFE-580TX 4 Port Server Adapter

        Click "Next" to continue.

     6. The wizard will copy and load the driver, than you will see "Finish"
        bottum. Click it and it's done.

 Driver keywords
 ---------------
     - Open 'Device Manager' in "My Computer" -> "Control Pannel" -> "System".
       Double click "D-Link DFE-580TX ...", Select "Advanced" item.

       Connection Type      Specify the connection type for the adapter.
                            Default: Auto-Negotiation

       Network Address      You can set the Ethernet address for your
                            adapter. It is not recommended to use this
                            keyword. As you know two or more adapter in
                            the same network with same Ethernet address
                            will cause a little problem.

                            When using this keyword you need to input
                            exactly 6 bytes of Ethernet address using
                            one of the following format:

                              xx-xx-xx-xx-xx-xx
                            OR
                              xxxxxxxxxxxx

                            Default: read address from adapter ROM.

       802.1Q/1P VLAN       You can enable it for VLAN group.
       tagging              Default: disable

       VLAN ID              This value will active after 802.1Q/1P VLAN
                            tagging enable.

       GVRP                 Support GVRP and will active after 802.1Q/1P
                            VLAN tagging enable.
                            Default: disable

