  Workstation for DOS ODI Client

  Introduction:
  -------------
  This document describes the procedure to setup the NetWare
  workstation driver for D-Link DGE-530T Gigabit Ethernet Adapter.

  Location of Driver: \DOSODI\D530ODI.COM

  Sample Configuration Files:
  ---------------------------
  STARTNET.BAT:
  LSL
  D530ODI
  IPXODI
  NETX or VLM

  NET.CFG:
  LINK DRIVER D530ODI
  MEDIUM AUTO --Specify adapter's speed. example
  --MEDIUM AUTO ;Auto negotiation
  --MEDIUM 1000FULL ;1000M FullDuplex
  --MEDIUM 100FULL ;100M FullDuplex
  --MEDIUM 100HALF ;100M HalfDuple
  --MEDIUM 10FULL ;10M FullDuplex
  --MEDIUM 10HALF ;10M HalfDuplex

  BUSNO NN --where NN is the PCI bus identifier of the PCI bus
  which connects to the adapter.
  DEVICENO NN --where NN is the specific PCI BIOS device
  identification number of the specified PCI adapter.
  [ or you can use "EtherID" to select a specific DGE-530T adapter:
  EtherID NNNNNNNNNNNN --Where NNNNNNNNNNNN specify a DGE-530T
  adapter's node address.This is only
  required when more than one DGE-530T
  adapters exist on one system.
  ]


  FRAME Ethernet_802.2 --Specify frame type
  FRAME Ethernet_802.3
  FRAME Ethernet_SNAP
  FRAME Ethernet_II

  NetWare DOS Requester
  FIRST NETWORK DRIVE = F
  NETWARE PROTOCOL = NDS BIND
  PREFERRED SERVER = NW5


  Setup Procedures for NetWare 3.11/3.12 Client:
  ----------------------------------------------
  Before you start with the installation process, make sure that
  the adapter is properly installed and configured. Make sure
  that your NetWare workstation is properly installed.

  1. Copy D530ODI.COM from the Realtek Driver Diskette subdirectory
  A:\DOSODI to your harddisk.

  2. Create a batch file, or add to your STARTNET.BAT file the commands
  listed above under STARTNET.BAT

  3. Edit the NET.CFG file that you copied over. Edit the file per your
  requirements (see examples above). If there are two frame types
  listed, whichever frame type is listed first, that is the one that
  the driver will load. See above for examples. The NET.CFG file
  should be in the same directory with the LSL.COM file.


  Setup Procedures for NetWare 4.X Client with vlm:
  -------------------------------------------------
  The installation utility INSTALL.EXE is located on NetWare's
  "Workstation for DOS" disk. Run INSTALL.EXE from the Workstation
  for DOS Disk.

  The NetWare Client Install program screen will appear. You must
  complete each of the questions. These options are specific to your
  needs.

  1. Enter the destination directory for the NetWare Client.
  (The default directory is C:\NWCLIENT).

  2. Gives you the option to automatically update the CONFIG.SYS
  and the AUTOEXEC.BAT files or modify them at a later time
  manually.

  3. Do you wish to install support for MS Windows ? (Y/N)
  (MS Windows Subdirectory: default C:\WINDOWS)

  4. Asks you to select a network driver and provide configuration
  options. It uses the specifications you select to create the
  file NET.CFG. Insert the DGE-530T drivers disk when prompted for
  the driver disk and specify the driver path A:\DOSODI

  5. Press <Enter> to install


  NOTE:
  -----
  1. Be sure to add LASTDRIVE=Z to your CONFIG.SYS file for the
  network mappings to work properly.

  2. When you have multiple DGE-530T Adapters on your system:
  Use "BUSNO" and "DEVICENO" KEYWORD in NET.CFG to select which
  adapter to use with your netware client.(or you can use "EtherID")

