
                  D-Link DGE-530T Gigabit Ethernet 10/100/1000 Adapter

 Contents
 --------
    - Introduction
    - Getting Started
    - Revision History
    - Copyrights, Trademarks, and Disclaimers

 Introduction
 ------------
    Thank you for purchasing the D-Link DGE-530T Gigabit Ethernet adapter.
    This CD-R driver support for the D-Link DGE-530T Gigabit Ethernet adapter
    (support 10M/100M/1000M PCI).
    
    This CD contains many kinds of Network Operating System 
    installation.  Please refer to the readme file or user's guide
    if any problems for installation, or please freely contact 
    our technical support.

    You can get latest releases of drivers from D-Link's Web site 
    (http://www.dlink.com). We hope our new readmes and installations
    will minimize the users effort to make our products work. Should there
    be further recommendations please contact the support manager at the
    local D-Link Office listed bellow.



 Getting Started
 ---------------
    Auto-run program assist your ease of setup.  It will configure
    driver, install appropriate network drivers for popular network
    operating systems on the DGE-530T adapter.


    You can operate some function through the friendly button:

    1.Install Driver: It will configure driver, install appropriate network drivers 
      for popular network operating systems on the DGE-530T adapter.
   
    2.Install SNMP Agent: It will install to the SNMP Agent for management.

    3.View Quick Installation Guide(PDF): It will show you how to install the hardware.
  
    4.View Manual(PDF): It will show detail manual for your reference.
   
    5.View SNMP Manual(PDF): It will show SNMP manual of installation for your reference.
    
    6.Install Acrobat Reader: You can install Acrobat Reader to read or print out your 
      user manual, and also many other applications.

    7.View Your Local D-Link Support: Please see the detail of our local branch office and
      contact our customer service window.

    8.Exit: You can exit Window by this button.
     
    If the NOS (Network Operating System) you are using is not covered
    by the auto-run program, please refer to the individual documentation
    provided in each NOS directory.


 Revisions History
 -----------------
    Revision 20080901
    -----------------
    --Including following drivers into NCU V2.11.9.3: 
      Microsoft Windows Server 2003 x86/x64
      Microsoft Windows XP x86/x64
      Microsoft Windows Vista x86/x64
      Microsoft Windows Server 2008 x86/x64
    --Update Microsoft Windows 2000 driver for WHQL Certificate
    --Update Manual
    


    Revision 20070715
    -----------------
    --Update Microsoft Vista x86/Vista x64/WinXP/2K/2003/2003 64bit/XP 64bit driver
    --Update Netware 5.X/6.X
    --Updaet Linux driver for Kernel 2.4.x/2.6.x
    --Add FreeBSD 6.0 driver
    --Update DOS ODI Client Drive/NDIS2/Client32 driver
    --Update Network Control Program
    --Update Manual/SNMP Manual
    --Update SNMP
    --Update QIG 

    Revision 20060101
    -----------------
    --Update all drivers for H/W rev. B1   
    --Add driver for Microsoft Windows XP 64 bit 
    

    Revision 20041001
    -----------------
    --Add driver for Microsoft Windows server 2003 
    --Update manual 


    Revision 20031015
    -----------------
    This version, provides partial release drivers for common NOSs.
    This CD-R includes:

    --Microsoft Windows 98SE/ NT4.0/ 2000/ ME /XP
    --Novell Netware 4.2/5.X/6.X/ ODI 1.11
    --Red Hat Linux 7.3 (kernel 2.4.18-3) or later

   
    Revision 20030815
    -----------------
    This is a preliminary version, provides partial release drivers for common NOSs.
    This CD-R includes:

    --Microsoft Windows 98SE/ NT4.0/ 2000/ ME /XP
    --Novell Netware 4.2/5.X/6.X/ ODI 1.11
    --Red Hat Linux 7.3 (kernel 2.4.18-3) or later
                   
 
    The BBS communication setup information is as follows :

    Speed     :  2400-14400  baud                           - Germany
                 2400-9600   baud                           - Asia,Taiwan
                 14400-16800 baud                           - Canada
                 9600-14400  baud V32, V32bis, V42, V42bis  - U.S.A.
                 2400-19200  baud V24, V32, V32bis, V42bis  - U.K. & Europe
    Parity    : none
    Data bits : 8
    Stop bit  : 1


 Copyrights, Trademarks, and Disclaimers
 ---------------------------------------
 All references to MS, Windows, Windows NT, WinNT are
 rights reserved by Microsoft Corporation
 
 All references to Nvl., ODI, Netware, NW, IPX, IPXODI, and LSL are
 rights reserved by Novell Corporation

 Further rights reserved to their respective corporations

