    ©Copyright 2002-2006 Marvell®.
    All rights reserved.

    m4cxw2k.htm created 22-Jun-2006

    Readme File for M4CXW2K.sys v8.39.10.3
    D-Link DGE-5xx Gigabit Ethernet Adapter

    NDIS5 Miniport Driver for Windows 2000 (x86)

# This file contains

1 Overview
2 Required Files
3 Installation

3.1 Installing the driver
3.2 Updating the driver

4 Parameters

## 1 Overview

    M4CXW2K.sys is the NDIS5 32-bit Miniport driver.

## 2 Required Files

    To install the driver, the following files are required:
    M4CXW2K.sys NDIS5 Miniport driver
    M4CXW2K.inf installation setup script
    M4CXW2K.CAT digital signature (only if the driver is certified)

## 3 Installation

3.1 Installing the driver

    Read the installation instructions in the adapter manual carefully.
    Follow these instructions to install the adapter in your computer.

    Due to the plug & play facility, the operating system is able to find,
    identify, and configure an adapter automatically.

    If the adapter is not detected during installation by the operating system the
    adapter is installed as "Ethernet Controller" under "Other Devices".
    To install the driver you have to perform a driver update as described
    in the next section.

3.2 Updating the driver

    To update the driver, proceed as follows:

    1.  On the desktop right click on MY COMPUTER.
    2.  Select MANAGE.
    3.  In the "Device Manager" select the adapter you wish to update.
    4.  Double click.
    5.  Select DRIVER.
    6.  Click UPDATE DRIVER ... .
    7. Follow the instructions given by the operating system to locate the driver.
    8.  If the driver which is found to be the latest is not the one you want
        to install, select the checkbox "Install one of the other drivers".
    9.  Click NEXT.
    10. Select the driver to be installed in the next listbox.
    11. Click NEXT.
        If a message is displayed saying that the driver is not digitally signed
        by Microsoft, click YES.
    12. The message "Windows has finished installing the software for this
        device" is displayed.
    13. Click FINISH to complete the installation.

    Please note that the latest version of the M4CXW2K driver is
    available for download from our web site.

## 4 Parameters

    The M4CXW2K.sys driver allows you to modify several options in order to
    optimize the operation of your adapter.

    1.  In "Network and Dial-up Connections" right click on the adapter you
        want to configure.
    2.  Select "Properties".
    3.  Click "Configure".
    4.  Click "Advanced".
    5.  In the "Property" box, select the option that you want to change.
    6.  Enter the desired value in the "Value" box.
    7.  When finished, click OK .
    The operating system will reload the driver with the changed settings.

    The parameters supported by the driver are described below.

    Network Address
    ------------------------
    Default value:  burned-in adapter address
    Valid range:    02-00-00-00-00-01 to FE-FF-FF-FF-FF-FF (hexadecimal),
                    where at least the "multicast" bit(Bit 0) must not be set
                    (it indicates that the address field contains an
                    individual address)and the "locally administered" bit (Bit 1)
                    is set (the address has been assigned by a local
                    administrator). These two bits are first and second
                    bits transmitted on the LAN medium.

    CAUTION: Each individual network MAC address can only be used once in a
             network. Assigning the same address to more than one adapter in
             the same network is not allowed and can cause serious network
             problems.

    To use a network MAC address other than the one burned into the adapter,
    enter the network address in the following hexadecimal format:

    	e.g.: 02-00-5A-98-12-34

    If the network address field blank is left blank (or a different number of
    digits is specified), the network address burned into the adapter will
    be used.

    Jumbo Frame Support
    ------------------------
    Default value: "Disabled"
    Valid values:
    	-"Disabled"
    	-"4088"
    	-"9014"

    This parameter specifies the frame size that the driver will support.
    The performance of your network usually increases If "Jumbo" frames are
    used. Do not enable this option if you are not sure that your network
    supports jumbo frames.

    Note: For Fast Ethernet adapters the valid range is limited to 1514.

    Hardware Checksuming
    ------------------------
    Default value: "On"
    Valid values:
    	-"On"
     	-"Off"

    This parameter is used to disable the hardware checksum offload for
    TCP/IP. There should be no need to disable checksum offload.

    Wake Up Capabilities
    ------------------------
    Default value: "Magic Packet and Pattern Magic"
    Valid values:
    	-"None"
    		wake on LAN capabilities are disabled
    	-"Magic Packet"
    		wake up with MagicPacket from ShutDown state,
    		OS Controlled from Hibernate or Standby state
    	-"Pattern Match"
    		wake up with a packet containing a special pattern
    		from ShutDown state, OS Controlled from Hibernate
    		or Standby state
    	-"Magic Packet and Pattern Match"
    		wake up with both from ShutDown state, OS Controlled
    		from Hibernate or Standby state
    	-"Link Change"
    		wake up with link change from ShutDown state,
    		OS Controlled from Hibernate or Standby state

    Wake From Shutdown
    ------------------------
    Default value: "Off"
    Valid values:
    	-"Off"
    		disable the capabilities of the NIC to wake the computer
    		from shutdown.
    	-"On"
    		enable the NIC to be capable to wake the computer from shutdown.

    Number of Receive Buffers
    ------------------------
    For Yukon family based ethernet controllers the following values are used:
    Default value:  50 (decimal)
    Valid range:    3..500 (decimal)

    For Yukon2 family based ethernet controllers the following values are used:
    Default value:  256 (decimal)
    Valid range:    256..512 (decimal)

    This parameters defines the number of receive buffers allocated by the
    driver. If the system does not have enough resources the driver will fail
    to load. Increasing this value may improve performance.

    Number of Transmit Buffers
    ------------------------
    For Yukon family based ethernet controllers the following values are used:
    Default value:  50 (decimal)
    Valid range:    4..200 (decimal)

    For Yukon2 family based ethernet controllers the following values are used:
    Default value:  256 (decimal)
    Valid range:    256..512 (decimal)

    This parameters defines the number of transmit buffers allocated by the
    driver. If the system does not have enough resources the driver will
    fail to load. Increasing this value may improve performance.

    Interrupt Moderation
    ------------------------
    Default value: "On"
    Valid values:
    	-"On"
    	-"Off"

    If more than the specified rate of interrupts occur, the function
    Interrupt Moderation groups these interrupts so that several data packets
    can be handled per interrupt. This will lead to lower CPU utilization
    but may increase the latency.

    Max IRQ per Sec
    ------------------------
    Default value:  5000 (decimal)
    Valid range:    1000..30000 (decimal)

    This parameter specifies the interrupt rate for Interrupt Moderation. If
    Interrupt Moderation is set to "Off" it will be ignored.

    Log Status Messages
    ------------------------
    Default value: "Status Messages"
    Valid values:
    	-"All Messages":
    		This option should only be used for test purposes.
    	-"Status Messages":
    		In this mode the driver will generate an event log
    		entry every time the link status changes.
    	-"Warnings":
    		In this mode you will only receive warning or error
    		messages.
    	-"Errors":
    		In this mode you will only receive error messages.
    	-"None":
    		All driver messages will be suppressed. It is not
    		recommended to use this value.

    This parameter specifies the messages, which are to be logged in the
    Event Log.

    Speed & Duplex
    ------------------------
    Default value: "Auto-Sense"
    Valid range:
    	-"Auto-Sense"
    	-"10Mbps Half Duplex"
    	-"10Mbps Full Duplex"
    	-"100Mbps Half Duplex"
    	-"100Mbps Full Duplex"
    	-"1000Mbps Full Duplex"

    The parameter "1000Mbps Full Duplex" is valid only for DGE530T adapter.
    This parameter contain information regarding autonegotiation,
    duplex capabilities and link speed. Only if the setting is "Auto" the
    Autonegotiation is set to "On", in every other settings it is turned "Off".

    NOTE: This parameter is not valid for fiber adapter.

    Preferred Port
    ------------------------
    Default value: "A"
    Valid range:
    	-"A"
    	-"B"

    NOTE: This parameter is only available for dual link adapters.

    Use this parameter to set the preferred port the RLMT (Redundant
    Link Management Technology) will use for all network traffic, if more than
    one port has an active link to the network.

    RLMT Mode
    ------------------------
    Default value: "CLS"
    Valid range:
    	-"CLS" (Check Link State):
    		RLMT uses the link state reported by the
     		adapter hardware for each individual port to determine whether a
     		port can be used for all network traffic or not.

    	-"CLP" (Check Local Port):
    		In this mode, RLMT monitors the network path
     		between the two ports of an adapter by regularly exchanging packets
    		between them. This mode requires a network configuration in which
    		the two ports "see" each other (i.e. there must not be any router
    		between the ports).

    	-"CLPSS" (Check Local Ports and Segmentation Status):
    		This mode supports
    		the same functions as the CLP mode and additionally checks network
    		segmentation by sending BPDU hello packets. Thus, this mode is only
    		to be used if Gigabit Ethernet switches are installed on the network
    		that have been configured to use the Spanning Tree protocol.

    NOTE: RLMT modes "CLP" and "CLPSS" are designed to operate in
          configurations where a network path between the ports on one adapter
          exists. Moreover, they are not designed to work where adapters are
          connected back-to-back.
          This parameter is only available for dual link adapters.

    802.1p Support
    ------------------------
    Default Value:	"Off"
    Valid Values:
    	-"Off"
    	-"On"

    This parameter will enable/disable the quality of service for specified
    port. By default this option is not enabled at the first install of
    the driver.

    BatteryModeLinkDetection
    ------------------------
    Default Value: "EnergyDetect+™"
    Valid Values:
    	-"NoEnergySaving":
    		No Energy saving functions are switched on in the NIC.

    	-"MaximumEnergySaving":
    		The NIC is switched off if there is no link in battery mode.
    		The driver wakes up the NIC every 20 seconds to check
    		if there is a new link.

    	-"EnergyDetect+™":
    		If battery-powered the NIC is set to "EnergyDetect+"™ mode.
    		The link is activated faster than in “MaximumEnergySaving" mode,
    		but the NIC requires more power.

    This parameter will set the mode in which the NIC is working if there
    is no link and the PC is battery-powered.

    BatterySpeedSettings
    ------------------------
    Default Value: "FullSpeed"
    Valid Values:
    	-"SmartSpeedDown":
    		If the computer is battery-powered, the NIC speed is
    		switched to 10/100Mbit/s to reduce the power consumption.

    	- "FullSpeed":
    		If the computer is battery-powered the NIC is working with
    		maximum speed and maximum power consumption.
    		If the computer is supplied by AC power all power saving features
    		are switched off, and the NIC is working with maximum speed.

    This parameter will sets the Line speed for the NIC if PC is
    battery-powered.

    FlowControl
    ------------------------
    Default value: "On"
    Valid range:
    	-"Off":
    		No link partner is allowed to send PAUSE frames.

    	-"On":
    		Both link partners are allowed to send PAUSE frames.

    This parameter can be used to set the flow control capabilities the port
    reports during auto-negotiation. This parameter can be set for each port
    individually, which is helpful if the port at the other end of the cable cannot
    handle all possible combinations. Using the default setting, the adapter should
    automatically detect the capabilities of the peer port.

    TCP Segmentation
    ------------------------
    Default value: "Enabled"
    Valid range:
    	-"Enabled":
    		The big packets are segmented on the NIC before to be sent to the
     		network. Using this method the processor will be not loaded to do
    		this job.

    	-"Disabled":
    		The packets are not segmented by the NIC.

    NOTE: 	This parameter is only available starting with the NICs based on
    		Yukon2 chip.

    *** End of Readme File ***