
           D-Link DHN-520 10Mb Home Phoneline NIC Installation
                        for Windows NT V4.0


 Getting Started
 ---------------

    - Please plug the adapter into PCI slot and start your Windows
      NT 4.0 normally.

    - Open "My Computer" -> "Control Panel" -> "Networks" icons.

    - Select "Adapter" -> "Add" -> "Have disk" items.
      Type the following.

            A:\         (A: is floppy drive)
                        OR
            D:\         (D: is CD drive)

      Select the "D-Link DHN-520 ...".

    - Windows NT 4.0 will copy the driver files from the driver disk.

    - After finishing file copy, Windows NT 4.0 will ask you to
      reboot the PC. Select YES.

    - Restart the computer.
