InS_StArT
DTTOK16.COM
1.0
^D-Link Token-Ring PCA 16/4 Adapter,DTTOK16.COM,IE0
^D-Link Token-Ring ISA 16/4 Adapter,DTTOK16.COM,IE0
^D-Link Token-Ring MC 16/4 Adapter,DTTOK16.COM,00M
^D-Link Token-Ring EISA 16/4 Adapter,DTTOK16.COM,0E0
^D-Link Token-Ring PCMCIA Card,DTTOK16.COM,IEM
?The driver can communicate across Source Routing bridges. To enable this, load the ROUTE.COM module after DTTOK16.COM
!OIEM(PORT)I/O Port
?If more than one Token-Ring 16/4 adapter is installed in the workstation, use the PORT parameter to identify the adapter. If no value is entered, the driver will search for an adapter and use the one at the lowest I/O Port address.
A20
A24
A50
A54
$OIEM(NODE ADDRESS)
400000000000
7FFFFFFFFFFF
$OIEM(MAX FRAME SIZE)Maximum Frame Size
?Maximum frame size accepted by the driver. The default is 4216.
632
8432
!OIEM(RECEIVE BUFFERS)Number of receive buffers
?This parameter is mainly for use with trace tools or other protocols expecting to receive frames back to back. By increasing the number to 2 or 4, the maximum frame rate obtainable is increased slightly. Each buffer is MAX FRAME SIZE long.
1
2
4
*OIEM(FRAME)
?Select the frame type(s) used by the protocols in the workstation. If no frame type(s) is specified, TOKEN-RING MSB will be supported. The LSB and MSB attributes are mutually exclusive and should not both be selected for the same frame type.
TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
InS_EnD
