# RP Update Additional Statistics

Use this to view Packet Control Function (PCF) and Service Option (SO) based RP Update Statistics.

## Procedure

To access RP Update Statistics information:

1. Right-click the device and select Monitor from the popup menu.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category menu.

3. Select any row and click on RP Update Statistics.

4. Select RP Update Additional Statistics from the Category menu.

The following information appears:

> Registration Acknowledgements Received (cCdmaPcfSoRpUpdRcvdAcks)

> Registration Acknowledgements Discarded (cCdmaPcfSoRpUpdDiscardedAcks)

> Lifetime Expiry Updates (cCdmaPcfSoRpUpdRpLifeExpReqs)

> PPP Termination Updates (cCdmaPcfSoRpUpdPPPtermReqs)

> Other Reason Updates (cCdmaPcfSoRpUpdOtherReaReqs)

### Registration Acknowledgements Received (cCdmaPcfSoRpUpdRcvdAcks)

Number of A11 registration acknowledgements received since system startup.

### Registration Acknowledgements Discarded (cCdmaPcfSoRpUpdDiscardedAcks)

Number of A11 registration acknowledgements discarded since system startup.

### Lifetime Expiry Updates (cCdmaPcfSoRpUpdRpLifeExpReqs)

Since system startup, the number of initial A11 registration updates sent due to RP lifetime expiry.

### PPP Termination Updates (cCdmaPcfSoRpUpdPPPtermReqs)

Since system startup, the number of initial A11 registration updates sent as a result of PPP termination.

### Other Reason Updates (cCdmaPcfSoRpUpdOtherReaReqs)

Since system startup, the number of initial A11 registration updates sent due to reasons other than RP lifetime expiry or PPP termination.