# CDMA PDSN PPP Authentication Statistics Contd

Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select CDMA PDSN PPP Authentication Statistics Contd from the Category list.

The following information appears:

> CHAP Authentication Timeout (cCdmaPppAuthChapTimeouts)

> PAP Authentication Timeout (cCdmaPppAuthPapTimeouts)

> MSCHAP Authentication Timeout (cCdmaPppAuthMschapTimeouts)

> PPP Authentication Skipped (cCdmaPppAuthSkips)

### CHAP Authentication Timeout (cCdmaPppAuthChapTimeouts)

The total number of PPP CHAP authentication timeouts due to the mobile node not responding to a CHAP request since the system was last restarted.

### PAP Authentication Timeout (cCdmaPppAuthPapTimeouts)

The total number of PPP PAP authentication timeouts due to the mobile node not sending a PAP request since the system was last restarted.

### MSCHAP Authentication Timeout (cCdmaPppAuthMschapTimeouts)

The total number of PPP MSCHAP authentication timeouts due to the mobile node not responding to a MSCHAP request since the system was last restarted.

### PPP Authentication Skipped (cCdmaPppAuthSkips)

The total number of PPP negotiations that skipped PPP authentication, since the system was last restarted.