# RP Registration Discard Statistics

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category list.

3. Select a row and click the RP Registration Statistics button.

4. Select RP Registration Discard Statistics from the Category list.

The following information appears:

> Initial A11 Registration Requests Discarded (cCdmaPcfSoRpInitRegDiscardedReqs)

> A11 Re-registration Requests Discarded (cCdmaPcfSoRpReRegDiscardedReqs)

> A11 De-registration Requests Discarded (cCdmaPcfSoRpDeRegDiscardedReqs)

> Handoff A11 Registration Requests Discarded (cCdmaPcfSoRpHandoffRegDiscardedReqs)

### Initial A11 Registration Requests Discarded (cCdmaPcfSoRpInitRegDiscardedReqs)

The number of initial A11 registration requests silently discarded since the system was last restarted.

### A11 Re-registration Requests Discarded (cCdmaPcfSoRpReRegDiscardedReqs)

The number of A11 re-registration requests silently discarded since the system was last restarted.

### A11 De-registration Requests Discarded (cCdmaPcfSoRpDeRegDiscardedReqs)

The number of A11 de-registration requests silently discarded since the system was last restarted.

### Handoff A11 Registration Requests Discarded (cCdmaPcfSoRpHandoffRegDiscardedReqs)

The number of handoff A11 registration requests silently discarded since the system was last restarted.