# GGSN Service Aware Statistics 1

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select GGSN Service Aware Statistics 1 from the Category list.

The following information appears:

> Service Aware APNs (cGgsnSANumServiceAwareApns)

> GGSN Events (cGgsnSATotalGgsnEvents)

> CSG Events (cGgsnSATotalCsgEvents)

> DCCA Events (cGgsnSATotalDccaEvents)

> Categories Created (cGgsnSATotalCreatedCategories)

> Synchronization Objects (cGgsnSATotalCreatedSyncObjs)

> Service Authorization (cGgsnSATotalServiceAuthMsgs)

> Service Stop (cGgsnSATotalServiceStopMsgs)

> Quota Granted (cGgsnSATotalQuotaGranted)

### Service Aware APNs (cGgsnSANumServiceAwareApns)

The number of service aware Access Point Names (APNs).

### GGSN Events (cGgsnSATotalGgsnEvents)

The number of GGSN events.

### CSG Events (cGgsnSATotalCsgEvents)

The number of Content Service Gateway events.

### DCCA Events (cGgsnSATotalDccaEvents)

The number of Diameter Credit Control Application (DCCA) events.

### Categories Created (cGgsnSATotalCreatedCategories)

The number of categories that are created. Categories will not be statically configured in GGSN. GGSN learns about the categories for a particular PDP session dynamically by the DCCA server and the Content Service Gateway.

### Synchronization Objects (cGgsnSATotalCreatedSyncObjs)

The number of synchronization objects that get created for each of the triggers, which keep track of the affected categories and their current state.

The synchronization object contains:

- Type of object.
- List of affected categories.

### Service Authorization (cGgsnSATotalServiceAuthMsgs)

The number of service authorization messages sent by the Content Service Gateway.

### Service Stop (cGgsnSATotalServiceStopMsgs)

The number of service stop messages received.

### Quota Granted (cGgsnSATotalQuotaGranted)

The total amount of quota granted.