# AAA Accounting Sessions

The AAA Accounting Sessions provides data for accounting sessions based on Authentication, Authorization, Accounting

## Procedure

1. Right-click the device, then select AAA.

2. Click Accounting Sessions.

The following information appears:

> Session Id (casnSessionId)

> User Id (casnUserId)

> IP Address (casnIpAddr)

> Idle Time (casnIdleTime)

> Disconnect (casnDisconnect)

> Call Id (casnCallTrackerId)

### Session Id (casnSessionId)

Identifies accounting protocol session.

A unique value within the system even if multiple accounting protocols are in use that corresponds to the following accounting protocol attributes:

RADIUS represents attribute 44, Acct-Session-Id

TACACS+ represents attribute 'task_id'

### User Id (casnUserId )

User login ID or zero length string if ID is unavailable.

Corresponds to following accounting protocol attributes:

RADIUS represents attribute 1, User-Name.

TACACS+ represents attribute 'user'.

### IP Address (casnIpAddr )

Session IP address or 0.0.0.0 if ID is not applicable or is unavailable.

RADIUS represents attribute 8, Framed-IP-Address.

TACACS+ represents attribute 'addr'.

### Idle Time (casnIdleTime )

Time elapsed since last user-level data was received or transmitted. Protocol level handshaking associated with call is idle.

### Disconnect (casnDisconnect )

End of session.

Setting value to true(1) initiates termination. Entry is removed after sesion ends. When entry is set to true(1), the termination process cannot be canceled by setting value false(2).

### Call Id (casnCallTrackerId )

Index entry value in CISCO-CALL-TRACKER-MIB cctActiveTable that corresponds to session.

Using this value to query cctActiveTable provides more detailed data about casnActiveEntry session.