# Mobile Router's Home Agent Address List

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Mobile Router's Home agent address list.

The following information appears:

> MN's HP IP Address (mnHAAddress)

> Priority for Home Agent (cmiMrHAPriority)

> Home Agent Best (cmiMrHABest)

> ##

## MN’s HA IP Address (mnHAAddress)

Mobile node home agent IP address.

### Priority for Home Agent (cmiMrHAPriority)

Priority for this home agent.

### Home Agent Best (cmiMrHABest)

Indicates whether this home agent is the best (in terms of the priority or the configuration time when multiple home agents have the same priority) or not. When true, the mobile router tries to register with this home agent first.