# Copy Config File

Device>Configure>File Copy>Copy Config File

Use the CiscoView Copy Config File window to copy config files to and from a remote host to runtime memory. Use these settings:

Protocol (fileCopyProtocol)

Use tftp or rcp for any remote copy.

From (fileCopyAction)

Use one of these options:

- Host to Runtime Copy the configuration file from host to runtime configuration over the network through tftp/rcp.

- Runtime to Host Copy the runtime configuration to host over the network through tftp/rcp.

Remote Host IP Address (fileCopyRemoteServer)

IP address of the tftp/rcp remote server from, or to which, a file is copied.

Source File Name (fileCopySrcFileName)

Source filename (including the path, if applicable) of file.

Destination File Name (fileCopyDstFileName)

Destination filename (including path, if applicable) of file.

rcp User Name (fileCopyUserName)

Remote user name for copy via rcp.

Copy part (fileCopyRuntimeConfigPart)

Indicates what part of the runtime configuration is to be copied.