# TCP Connection Table

## Navigation

1. Right-click on the Persistent Storage Device (PSD) card and then select PSD Details.

2. In the contents pane, double-click on the Network Details folder and then select TCP Connection Table.

The TCP Connection Table dialog box provides information on the TCP connections configured in this system.

This dialog box displays the following data:

- Local Address (tcpConnLocalAddress)

- Local Port (tcpConnLocalPort)

- Remote Address (tcpConnRemAddress)

- Remote Port (tcpConnRemPort)

- Connection State (tcpConnState)

Local Address (tcpConnLocalAddress)

Local IP address of this TCP connection.

For connections in the listen state which accept connections from any IP interface associated with the node, the value 0.0.0.0 is used.

Local Port (tcpConnLocalPort)

Local port number of this TCP connection.

Remote Address (tcpConnRemAddress)

Remote IP address of this TCP connection.

Remote Port (tcpConnRemPort)

Remote port number of this TCP connection.

Connection State (tcpConnState)

State of this TCP connection.