# SSG Excluded APN Table

This dialog box displays details on the Service Selection Gateway (SSG) excluded access point name (APN).

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Excluded APN Table from the Category list.

### Excluded APN (cssgExcludedAPNName)

Name of the excluded APN.

### APN Row Status (cssgExcludedAPNRowStatus)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

- To delete a row, set the object to destroy.