# CSG Global Statistics

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.
3. With a device selected, click Statistics.
4. Select Content Services Gateway from the Category drop-down box.
5. Select CSG Global Statistics from the Category drop-down box.

The following information appears:

> Active Session Users (ccsgsUserCurrent)

> User Reset Time (ccsgsUserHighWaterResetTime)

> Total Sessions (ccsgsSessionCurrent)

> Session Reset Time (ccsgsSessionHighWaterResetTime)

### Active Session Users (ccsgsUserCurrent)

Total number of users with one or more active sessions on the system.

### User Reset Time (ccsgsUserHighWaterResetTime)

Indicates when the ccsgsUserHighWater object was last reset to zero.

### Total Sessions (ccsgsSessionCurrent)

Total number of sessions on the system. A session corresponds to a TCP/UDP flow.

### Session Reset Time (ccsgsSessionHighWaterResetTime)

Indicates when the ccsgsSessionHighWater object was last reset to zero.