# Home Agent Registration Statistics Per Node

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select Home Agent Registration Table.

4. With an entry selected in the Home Agent Registration table, click Monitor.

The following information is displayed:

> Accepted Requests Count (haServiceRequestsAccepted)

> Denied Requests Count (haServiceRequestsDenied)

> Overall Service Time (haOverallServiceTime)

### Accepted Requests Count (haServiceRequestsAccepted)

Total number of service requests for the mobile node accepted by the home agent (code 0 + code 1).

### Denied Requests Count (haServiceRequestsDenied)

Total number of service requests for the mobile node denied by the home agent (sum of all registrations denied with code 128 through 159).

### Overall Service Time (haOverallServiceTime)

Overall service time, in seconds, that have been accumulated for the mobile node since the home agent last rebooted.