# SSG Port Server Association

The SSG Port Server Association category of the Configure dialog box displays details on the service selection gateway (SSG) port server association.

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG Port Server Association from the Category list.

The following information appears:

Redirect-Group Name (cssgTcpRedirectGrpName)

Server Group Port Number (cssgTcpRedirPortNo)

Port Server Association RowStatus (cssgTcpRedirPortNoMapRowStat)

### Redirect-Group Name (cssgTcpRedirectGrpName)

Name of the redirect group.

### Server Group Port Number (cssgTcpRedirPortNo)

Port number associated with the server group.

### Port Server Association RowStatus (cssgTcpRedirPortNoMapRowStat)

Status of the table entry.

Status can be used to create or delete conceptual rows in the table.

To create a row, set the object to createAndGo. cssgTcpRedirPortNo is a mandatory object for a create request.

To delete a row, set the object to destroy.