# Mobile IP Notification Related Object Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Mobile IP Notification Related Object Configs.

The following information appears:

> Mobile IP Notification (cmiTrapControl)

> CoAType (cmiNtRegCOAType)

> Mobile Node's Care-of Address (cmiNtRegCOA)

> HA Address Type (cmiNtRegHAAddrType)

> Mobile Node's Home Agent Address (cmiNtRegHomeAgent)

> Registered Home Address Type (cmiNtRegHomeAddressType)

> Visiting Mobile Node Home (IP) Address (cmiNtRegHomeAddress)

> Reg NAI (cmiNtRegNAI)

> Registration Deny Reason (cmiNtRegDeniedCode)

### Mobile IP Notification (cmiTrapControl)

Turns mobile IP notification generation on and off . Setting a notification type's bit to:

1 | Enables generation of notifications of that type, subject to further filtering resulting from entries in the snmpNotificationMIB.
0 | Disables generation of notifications of that type.

### CoAType (cmiNtRegCOAType)

Type of the address stored in cmiHaRegMnCOA.

### Mobile Node's Care-of Address (cmiNtRegCOA)

Mobile node's care-of address.

### HA Address Type (cmiNtRegHAAddrType)

Type of the address stored in cmiHaRegMnHa.

### Mobile Node's Home Agent Address (cmiNtRegHomeAgent)

Mobile node's home agent address.

### Registered Home Address Type (cmiNtRegHomeAddressType)

Type of the address stored in cmiHaRegRecentHomeAddress.

### Visiting Mobile Node Home (IP) Address (cmiNtRegHomeAddress)

Home (IP) address of visiting mobile node.

### Reg NAI (cmiNtRegNAI)

Identifier associated with the mobile node.

### Registration Deny Reason (cmiNtRegDeniedCode)

Code indicating the reason that the most recent Registration Request for this mobile node was rejected by the home agent.