# PPPoE VCL Session-Exceeded VCL Sessions

The PPPoE VCL (Virtual Circuit Link) Session-Exceeded System Sessions dialog box monitors the exceeded sessions error for the specified interval for this VCL. The unit is "attempts/interval".

## Procedure

1. Right-click the device, then select PPPoE.

2. Select a row from VCL Session Info Table, then click VCL Sessions.

3. Choose the required VCL and click Monitor Exceeded Session Errors.

The following information appears:

> Exceeded Sessions Error (cPppoeVcExceededSessionErrors )

### Exceeded Sessions Error (cPppoeVcExceededSessionErrors)

The accumulated number of errors for establishing PPPoE session in the VC due to the cPppoeVcCurrSessions value exceeds the cPppoeVcMaxAllowedSessions value.