# Home Agent Registration Processing Statistics - Registration Requests

## Navigation

1. ## Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. ## Select Home Agent Registration Processing Statistics – Registration Requests from the Category list.

The following information appears:

> Registration Requests (cmiHaRegTotalProcLocRegs)

> Max Requests (cmiHaRegMaxProcLocInMinRegs)

> Requests Processed (cmiHaRegProcLocInLastMinRegs)

> Processed by HA (cmiHaRegTotalProcByAAARegs)

> Max Processing by HA (cmiHaRegMaxProcByAAAInMinRegs)

> Last Minute Processing by HA (cmiHaRegProcAAAInLastByMinRegs)

> Requests Received by HA (cmiHaRegRequestsReceived)

> Requests Denied by HA (cmiHaRegRequestsDenied)

> Requests Discarded by HA (cmiHaRegRequestsDiscarded)

### Registration Requests (cmiHaRegTotalProcLocRegs)

The total number of registration requests processed by the home agent. Includes only those registration requests that were authenticated locally by the home agent.

### Max Requests (cmiHaRegMaxProcLocInMinRegs)

The maximum number of registration requests processed in a minute by the home agent. Includes only those registration requests that were authenticated locally by the home agent.

### Requests Processed (cmiHaRegProcLocInLastMinRegs)

The number of registration requests processed during the last minute by the home agent. Includes only those registration requests that were authenticated locally by the home agent.

### Processed by HA (cmiHaRegTotalProcByAAARegs)

The total number of registration requests processed by the home agent. Includes only those registration requests that were authenticated by the AAA server.

### Max Processing by HA (cmiHaRegMaxProcByAAAInMinRegs)

The maximum number of registration requests processed in a minute by the home agent. Includes only those registration requests that were authenticated by the AAA server.

### Last Minute Processing by HA (cmiHaRegProcAAAInLastByMinRegs)

The number of registration requests processed by the home agent in the last minute. Includes only those registration requests that were authenticated by the AAA server.

### Requests Received by HA (cmiHaRegRequestsReceived)

The total number of registration requests received by the home agent. Includes initial registration requests, re-registration requests, and de-registration requests.

### Requests Denied by HA (cmiHaRegRequestsDenied)

The total number of registration requests denied by the home agent. Reasons for which a home agent denies a request include:

1. Cannot allocate IP address for mobile node.
2. Request parsing failed.
3. NAI length exceeds the packet length.

### Requests Discarded by HA (cmiHaRegRequestsDiscarded)

The total number of registration requests discarded by the home agent. Reasons for which a home agent discards a request include:

1. IP mobile home agent service not enabled.
2. HA-CHAP authentication failed.
3. Mobile node security association retrieval failed.