# Destination Profile Table

## Navigation

Right-click the device and then select Configure > System Log > Call Home Facility > Destination Profile Table.

The following information is displayed:

- Call Home Message Format (callHomeDestProfileMsgFormat)

- Message Size (callHomeDestProfileMaxMsgSize)

- Message Transport Method (callHomeDestProfileTrnsprtMthd)

### Call Home Message Format (callHomeDestProfileMsgFormat)

CallHome format used by this profile when sending messages. Implementations are allowed to assign a default value.

### Message Size (callHomeDestProfileMaxMsgSize)

Maximum size of messages that can be sent by this destination profile. Implementations are allowed to assign a default value.

When the value of this object is zero, there is no limit on the size of messages sent by this destination profile.

### Message Transport Method (callHomeDestProfileTrnsprtMthd)

CallHome transport method used to deliver alert messages.