# Server Farm Info

To access the Server Farm Info dialog box:

1. Select Device > Configure > SLB Statistics.

2. With a server load balancing (SLB) instance selected, click Server Farm.

This dialog box provides details about the server farms, like the name of the server farm, details of the algorithm configured on the server farm, bind identification number, and the number of real servers present in the server farm.

The Server Farm Info dialog box displays the following data:

- Farm Name (slbServerFarmName)

- Farm Predictor (slbServerFarmPredictor)

- Nat (slbServerFarmNat)

- No. of Real Servers (slbServerFarmNumberOfRealServers)

- Bind Identification (slbServerFarmBindId)

- Server Row Status (slbServerFarmRowStatus)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Farm Name (slbServerFarmName)

The name of the server farm.

Farm Predictor (slbServerFarmPredictor)

The load balancing algorithm used by the server farm for its real servers for the local SLB entity.

Nat (slbServerFarmNat)

The type of network address translation (NAT) employed by the local SLB entity for servers in this server farm.

No. of Real Servers (slbServerFarmNumberOfRealServers)

The number of real servers in the server farm.

Bind Identification (slbServerFarmBindId)

Bind Identification is used to identify one or more real servers for which slbDfpRealWeight applies to the slbRealOperWeight of the real server.

Rows in slbServerFarmTable for which slbServerFarmBindId matches slbDfpRealBindId are identified.

Server Row Status (slbServerFarmRowStatus)

The management station uses row status to create or delete the row entry in slbServerFarmTable following the RowStatus textual convention.