# DFP Agent Info

This dialog box provides information about the Dynamic Feedback Protocol (DFP) agents that reports to the server load balancing (SLB) managers.

## Procedure

1. Right-click the device, then select Configure > SLB Statistics.

2. With a server load balancing (SLB) instance selected, click DFP Agents. The following information is displayed.

> DFP Agent IP Address (slbDfpAgentIpAddress)

> DFP Agent Port (slbDfpAgentPort)

> DFP Agent State (slbDfpAgentState)

> Timeout (slbDfpAgentTimeout)

> Manager Retry count (slbDfpAgentRetryCount)

> Retry interval (slbDfpAgentInterval)

> DFP Agent Row status (slbDfpAgentRowStatus)

### DFP Agent IP Address (slbDfpAgentIpAddress)

The IP address of the DFP agent.

### DFP Agent Port (slbDfpAgentPort)

The port of the DFP agent.

### DFP Agent State (slbDfpAgentState)

The state of the DFP agent.

### Timeout (slbDfpAgentTimeout)

The time interval during which the agent must send at least one message to the manager.

### Manager Retry count (slbDfpAgentRetryCount)

The number of times the manager attempts to reestablish a connection with the agent.

### Retry interval (slbDfpAgentInterval)

The time interval before SLB retries connecting to a DFP.

### DFP Agent Row status (slbDfpAgentRowStatus)

A management station uses row status to create or delete the row entry in slbDfpAgentTable following the RowStatus textual convention.