# Home Agent Registration Table

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select Home Agent Registration Table.

The following information is displayed:

> MN Ip Address (haMobilityBindingMN)

> Latest Regn Accepted Time (haRecentServiceAcceptedTime)

> Latest Regn denied Time (haRecentServiceDeniedTime)

> Latest Regn denied Code (haRecentServiceDeniedCode)

### MN Ip Address (haMobilityBindingMN)

Home IP address of the mobile node.

### Latest Regn Accepted Time (haRecentServiceAcceptedTime)

The time when the most recent registration request was accepted by the home agent for a mobile node.

### Latest Regn denied Time (haRecentServiceDeniedTime)

The time when the most recent registration request was denied by the home agent for a mobile node.

### Latest Regn denied Code (haRecentServiceDeniedCode)

Code indicating the reason for the rejection of the registration request by the home agent. Possible values include:

> reasonUnspecified(128)

> admProhibited(129)

> insufficientResource(130)

> mnAuthenticationFailure(131)

> faAuthenticationFailure(132)

> idMismatch(133)

> poorlyFormedRequest(134)

> tooManyBindings(135)

> unknownHA(136)