# CDMA PDSN Update Statistics

Use this option to view valid and accepted registration updates.

## Procedure

To access CDMA PDSN update statistics information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

2. Select CDMA PDSN Update Statistics from the Category menu.

CDMA PDSN Update Statistics dialog box displays:

Registration Update Request Transmitted (cCdmaRpUpdTransmittedReqs)

Registration Update Request Accepted (cCdmaRpUpdAcceptedReqs)

Registration Update Request Denied (cCdmaRpUpdDeniedReqs)

Registration Update Request Not Acknowledged (cCdmaRpUpdNotAckedReqs)

Initial Registration Update Requests (cCdmaRpUpdInitTransmittedReqs)

Retransmitted Registration Update Requests (cCdmaRpUpdReTransmittedReqs)

### Registration Update Request Transmitted (cCdmaRpUpdTransmittedReqs)

Number of A-11 registration updates transmitted since system startup.

### Registration Update Request Accepted (cCdmaRpUpdAcceptedReqs)

Number of A-11 registration acknowledgements received since system startup with status field set to zero (indicating that the corresponding registration update is accepted).

### Registration Update Request Denied(cCdmaRpUpdDeniedReqs)

Number of A-11 registration acknowledgements received with status field set to non-zero (indicating that the corresponding registration update is denied), since system startup.

### Registration Update Request Not Acknowledged(cCdmaRpUpdNotAckedReqs)

Number of A-11 registration updates sent, for which no A-11 registration acknowledgements are received, since system startup.

### Initial Registration Update Requests (cCdmaRpUpdInitTransmittedReqs)

Numberof initial A-11 registration updates sent since system startup excluding the re-transmitted A-11 registration updates.

### Retransmitted Registration Update Requests (cCdmaRpUpdReTransmittedReqs)

Number of re-transmitted A-11 registration updates since system startup.