# CDMA PDSN PPP Setup Failures

Use this option to view PPP requests that are rejected.

## Procedure

To access CDMA PDSN PPP setup failure information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

2. Select CDMA PDSN PPP Setup Failures from the Category menu.

CDMA PDSN PPP Setup Failures dialog box displays:

PPP Connection Setup Reqs Failed (cCdmaPppConnectionFailures)

PPP Connections Failed at LCP stage (cCdmaPppLcpFailures)

PPP Connections Failed at AUTH stage (cCdmaPppAuthFailures)

PPP Connections Failed at IPCP stage (cCdmaPppIpcpFailures)

Note: The following variables are available for PSDNv2.0.

LCP Stage Failures after Maximum Retransmission(cCdmaPppLcpFailuresMaxRetrans)

LCP Stage Failures Due to Unknown Reason(cCdmaPppLcpFailuresUnknown)

IPCP Stage Failures after Maximum Retransmission (cCdmaPppIpcpFailuresMaxRetrans)

IPCP Stage Failures Due to Unknown Reason (cCdmaPppIpcpFailuresUnknown)

PPP Negotiations Aborted Prematurely (cCdmaPppConnectionsAborted)

### PPP Connection Setup Reqs Failed (cCdmaPppConnectionFailures)

Number of times PPP connection setup requests failed since system startup.

### PPP Connections Failed at LCP stage (cCdmaPppLcpFailures)

Number of times PPP connection requests failed at LCP stage since system startup.

### PPP Connections Failed at AUTH stage (cCdmaPppAuthFailures)

Number of times PPP setup connections failed at authentication stage since system startup.

### PPP Connections Failed at IPCP stage (cCdmaPppIpcpFailures)

Number of times PPP setup connections failed at IPCP stage since system startup.

### LCP Stage Failures after Maximum Retransmission (cCdmaPppLcpFailuresMaxRetrans)

Since system startup, the number of PPP connection requests that failed at LCP stage after the maximum number of retransmissions.

### LCP Stage Failures Due to Unknown Reason (cCdmaPppLcpFailuresUnknown)

Since system startup, the number of PPP connection requests that failed at LCP stage due to an unknown reason.

### IPCP Stage Failures after Maximum Retransmission (cCdmaPppIpcpFailuresMaxRetrans)

Since system startup, the number of PPP connection requests that failed at IPCP stage after maximum number of retransmission.

### IPCP Stage Failures Due to Unknown Reason (cCdmaPppIpcpFailuresUnknown)

Since system startup, the number of PPP connection requests that failed at IPCP stage due to an unknown reason.

### PPP Negotiations Aborted Prematurely (cCdmaPppConnectionsAborted)

Since system startup, the number of PPP negotiations that terminated prematurely due to MN power-off.