# Invalid RP Registration Update Ack Errors Stats

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Statistics button.
4. Select category Invalid RP Registration Update Ack Errors Stats.
5. Select a row and click on Monitor.

The following information appears:

> Invalid Registration Update (cCdmaRegUpdAckInvPakLenErrs )

> Invalid Protocol Value (cCdmaRegUpdAckInvProtocolErrs)

> Invalid Authentication Key (cCdmaRegUpdAckInvRUAEKeyErrs)

> Invalid SPI (cCdmaRegUpdAckInvSPIErrs)

> Invalid Connection ID (cCdmaRegUpdAckInvConnectionIDErrs)

> Invalid MN ID (cCdmaRegUpdAckInvMNIDErrs)

> Invalid MN ID Type (cCdmaRegUpdAckInvMNIDTypeErrs)

> Invalid MSID Length (cCdmaRegUpdAckInvMSIDLenErrs)

### Invalid Registration Update (cCdmaRegUpdAckInvPakLenErrs )

Number of Invalid Registration Update Ack packet length while parsing since the system was last restarted.

### Invalid Protocol Value (cCdmaRegUpdAckInvProtocolErrs)

Number of Invalid Protocol value in the Registration Update Ack Session Specific Extension since the system was last restarted.

### Invalid Authentication Key (cCdmaRegUpdAckInvRUAEKeyErrs)

Number of Invalid Authentication key in the Registration Update Ack Registration Update Authentication extension since the system was last restarted.

### Invalid SPI (cCdmaRegUpdAckInvSPIErrs)

Number of Invalid SPI in the Registration Update Ack Registration Update Authentication extension since the system was last restarted.

### Invalid Connection ID (cCdmaRegUpdAckInvConnectionIDErrs)

Number of Invalid Connection ID in the Registration Update Ack since the system was last restarted.

### Invalid MN ID (cCdmaRegUpdAckInvMNIDErrs)

Number of Invalid MN ID in the Registration Update Ack since the system was last restarted.

### Invalid MN ID Type (cCdmaRegUpdAckInvMNIDTypeErrs)

Number of Invalid MN ID type in the Registration Update Ack since the system was last restarted.

### Invalid MSID Length (cCdmaRegUpdAckInvMSIDLenErrs)

Number of Invalid MSID length in the Registration Update Ack since the system was last restarted.