# Interface Capabilities

Configuration > Global > Interface Capabilities

This dialog box displays a list of interfaces with their corresponding traffic direction, queue type, and capabilities.

To set the capabilities for a particular interface, click the corresponding entry for that interface in the Capabilities column, which brings up the Bits Property dialog box.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Interface (ifIndex)

- Direction (Direction)

- Queue Type (QosInterfaceQueueType)

- Capabilities (QosInterfaceTypeCapabilities)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

Interface (ifIndex)

A unique value, greater than zero, for each interface.

Direction (Direction)

Indicates a particular direction of traffic.

Queue Type (QosInterfaceQueueType)

An enumerated type for all known interfaces.

Capabilities (QosInterfaceTypeCapabilities)

An enumeration of interface capabilities.