# GGSN Access Point Violation and Redirection

Use this dialog to view access point violation and inter mobile redirection statistics.

## Procedure

1. Right-click the device and then select Monitor.

2. Select GGSN Access Point Statistics from the Category list.

3. Select a row and click on Monitor.

4. Select category GGSN Access Point Violation and Redirection.

The following information appears:

> Source Address Violation (cgprsAccPtSourceAddrViolTpdus)

> Destination Address Violation (cgprsAccPtDestAddrViolTpdus)

> Redirected InterMobile Communication (cgprsAccPtRedirInterMobilTraffic)

### Source Address Violation (cgprsAccPtSourceAddrViolTpdus)

Number of upstream TPDU's (Payload of GPRS Tunneling Protocol) that have been dropped due to source address violation as specified by cgprsAccPtVerifyUpStrTpduSrcAddr.

### Destination Address Violation (cgprsAccPtDestAddrViolTpdus)

Number of upstream TPDU's that have been dropped due to destination address violation as specified by cgprsAccPtVerifyUpStrTpduDstAddr.

### Redirected InterMobile Communication (cgprsAccPtRedirInterMobilTraffic)

Number of packets, pertaining to inter obile communication, that have been redirected to the device specified by cgprsAccPtRedirInterMobilAddr.