# RP Registration Reply Errors

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select category RP Registration Reply Errors.

5. Select a row and click on Monitor.

The following information appears:

> Internal Error (cCdmaRegRplyInternalErrs)

> Memory Allocation Failure (cCdmaRegRplyMemFailErrs)

> Security Association Not found or Parse Error (cCdmaRpRplyPCFNoSecOrParseErrs)

### Internal Error (cCdmaRegRplyInternalErrs)

Number of registration replies not sent due to internal errors during processing since the system was last restarted

### Memory Allocation Failure (cCdmaRegRplyMemFailErrs)

Number of registration replies not sent due to memory allocation failures during processing since the system was last restarted.

### Security Association Not found or Parse Error (cCdmaRpRplyPCFNoSecOrParseErrs)

Number of Cannot send Reply to PCF due to security association not found for the PCF or Parse error of Request since system was last restarted.