# RP Update Additional Statistics

From this dialog box, you can view Packet Control Function (PCF) and Service Option (SO)-based RP update statistics.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PCF & SO Based Statistics.

4. With an entry selected in the PCFs & Service Options table, click RP Update Statistics.

5. Select RP Update Additional Statistics.

The following information is displayed:

> Registration Acknowledgements Received (cCdmaPcfSoRpUpdRcvdAcks)

> Registration Acknowledgements Discarded (cCdmaPcfSoRpUpdDiscardedAcks)

> Lifetime Expiry Updates (cCdmaPcfSoRpUpdRpLifeExpReqs)

> PPP Termination Updates (cCdmaPcfSoRpUpdPPPtermReqs)

> Other Reason Updates (cCdmaPcfSoRpUpdOtherReaReqs)

### Registration Acknowledgements Received (cCdmaPcfSoRpUpdRcvdAcks)

Number of A11 registration update acknowledgements received since system startup.

### Registration Acknowledgements Discarded (cCdmaPcfSoRpUpdDiscardedAcks)

Number of A11 registration update acknowledgements discarded since system startup.

### Lifetime Expiry Updates (cCdmaPcfSoRpUpdRpLifeExpReqs)

Number of initial A11 registration update requests sent due to RP lifetime expiry since system startup.

### PPP Termination Updates (cCdmaPcfSoRpUpdPPPtermReqs)

Number of initial A11 registration update requests sent as a result of PPP termination since system startup.

### Other Reason Updates (cCdmaPcfSoRpUpdOtherReaReqs)

Number of initial A11 registration update requests sent due to reasons other than RP lifetime expiry or PPP termination since system startup.