# Quota Managers Statistics

From this dialog box, you can monitor the traffic statistics for the selected quota manager in real time.

## Navigation

1. Right-click the device, then select Configure > Content Services Gateway.

2. With a content services gateway (CSG) module selected, click Quota Managers.

3. With a quota manager selected, click Monitor.

The following information is displayed:

> Lost Records (csgQuotaMgrLostRecords)

> Records Sent (csgQuotaMgrTotalSent)

> ACKs. Failed (csgQuotaMgrFailAck)

> Msgs to be ACKed (csgQuotaMgrOutstanding)

> Quota Mgr. High Water (csgQuotaMgrHighWater)

> Bad Records Received (csgQuotaMgrBadRecord)

> Msgs. Retransmitted (csgQuotaMgrRetransmit)

### Lost Records (csgQuotaMgrLostRecords)

Total number of records lost since system initialization or the last time the counter wrapped.

### Records Sent (csgQuotaMgrTotalSent)

Total number of records sent to the quota manager.

### ACKs. Failed (csgQuotaMgrFailAck)

Number of acknowledgments received from the quota manager for which there are no requests.

### Msgs to be ACKed (csgQuotaMgrOutstanding)

Current number of messages waiting to be acknowledged.

### Quota Mgr. High Water (csgQuotaMgrHighWater)

Highest number of messages waiting for acknowledgment. The only write operation allowed for this object is to reset its value to zero.

### Bad Records Received (csgQuotaMgrBadRecord)

Number of bad records received. These are records in which the CSG detected an error while attempting to decode the contents.

### Msgs. Retransmitted (csgQuotaMgrRetransmit)

Number of messages retransmitted to the billing mediation agent (BMA).