# PSD Server

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select PSD Server from the Category list.

The following information appears:

> Data-Store Name (cPsdClientDSName)

> PSD Server Address Type (cPsdClientDSServerAddressTyp)

> PSD Server Address (cPsdClientDSServerAddress)

> Write/Retrievable Service (cPsdClientDSRetrieveOnly)

> Server Row Status (cPsdClientDSServerRowStatus)

### Data-Store Name (cPsdClientDSName)

The name of the configured data-store.

### PSD Server Address Type (cPsdClientDSServerAddressTyp)

The type of Internet address of the PSD server.

### PSD Server Address (cPsdClientDSServerAddress)

The Internet address of the PSD server.

### Write/Retrievable Service (cPsdClientDSRetrieveOnly)

Indicates whether the PSD server can be configured as retrievable only or as write/retrievable. When set to true, the PSD server (the value of the corresponding instance of cPsdClientDSServerAddress) cannot be used for writing Call Detail Records (CDRs). When set to false, the PSD server can be used for writing CDRs as well as for retrieving them.

### Server Row Status (cPsdClientDSServerRowStatus)

Creates a row or deletes an existing row in a table.