# CDMA PDSN PCF and Service Option-Based RP Session Update Statistics Contd

1. Right click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Configure button.
4. Select category CDMA PDSN PCF and Service Option based RP Session Update.
5. S elect a row.

   Note: Clicking the Monitor1 button displays information for CDMA PDSN PCF and Service Option based RP Session Update Statistics. Clicking the Monitor 2 button displays information for CDMA PDSN PCF and Service Option based RP Session Update Statistics Contd.

6. Click the Monitor2 button.

The following information appears:

> Always On Registration Updates (cCdmaPcfSoRpSessUpdAlwaysOn)

> TNPDIT download Registration Updates (cCdmaPcfSoRpSessUpdRNPDIT)

> Session Parameter not Updated (cCdmaPcfSoRpSessUpdParamNotUpdated)

> Unspecified Reason Failures (cCdmaPcfSoRpSessUpdReaUnSpecFails)

> MN Authentication Failure (cCdmaPcfSoRpSessUpdMNAuthFails)

> Registration Identity Mismatch (cCdmaPcfSoRpSessUpdIdMismatFails)

> Poorly Formed Request (cCdmaPcfSoRpSessUpdBadReqFails)

### Always On Registration Updates (cCdmaPcfSoRpSessUpdAlwaysOn)

Total number of initial A11 registration updates sent due to Always On downloaded since the system was last restarted.

### TNPDIT download Registration Updates (cCdmaPcfSoRpSessUpdRNPDIT)

Total number of initial A11 registration updates sent due to TNPDIT downloaded since the system was last restarted.

### Session Parameter not Updated (cCdmaPcfSoRpSessUpdParamNotUpdated)

Number of session updates that failed for session parameter not updated reason since the system was last restarted.

### Unspecified Reason Failures (cCdmaPcfSoRpSessUpdReaUnSpecFails)

Number of session updates that failed for unspecified reason since the system was last restarted.

### MN Authentication Failure (cCdmaPcfSoRpSessUpdMNAuthFails)

Number of session updates that failed due to MN authentication failure since the system was last restarted.

### Registration Identity Mismatch (cCdmaPcfSoRpSessUpdIdMismatFails)

Number of session updates that failed due to registration identity mismatch since the system was last restarted.

### Poorly Formed Request (cCdmaPcfSoRpSessUpdBadReqFails)

Number of session updates that failed due to poorly formed request since the system was last restarted.