# Home Agent Registration Processing Configs

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Home Agent Registration Processing Configs from the Category list.

The following information appears:

> Max Registration Processed (cmiHaRegDateMaxRegsProcLoc)

> Max Registration Processed by AAA (cmiHaRegDateMaxRegsProcByAAA)

> Average Processing Time (cmiHaRegAvgTimeRegsProcByAAA)

> Maximum Processing Time (cmiHaRegMaxTimeRegsProcByAAA)

### Max Registration Processed (cmiHaRegDateMaxRegsProcLoc)

The time at which the number of registration requests processed in a minute by the home agent reached maximum. Includes only those registration requests that were authenticated locally by the home agent.

### Max Registration Processed by AAA (cmiHaRegDateMaxRegsProcByAAA)

The time at which number of registration requests processed in a minute by the home agent reached maximum. Includes only those registration requests that were authenticated by the AAA server.

### Average Processing Time (cmiHaRegAvgTimeRegsProcByAAA)

The average time taken by the home agent to process a registration request. Calculated based on those registration requests that were authenticated by the AAA server only.

### Maximum Processing Time (cmiHaRegMaxTimeRegsProcByAAA)

The maximum time taken by the home agent to process a registration request. It considers only those registration requests that were authenticated by the AAA server.