# CDMA PDSN PPP Normal Release Statistics

This dialog box is applicable to Member and Peer to Peer clusters. From here, you can view point-to-point protocol (PPP) statistics for a release.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PPP Normal Release Statistics.

The following data is displayed:

> Total PPP Connections Released (PDSN or MS) (cCdmaPppTotalReleases)

> PPP Connections Released by PDSN (cCdmaPppPdsnReleases)

> PPP Connections Released by Mobile (cCdmaPppMobileReleases)

> PPP Released Due to Ingress Addr Filtering (cCdmaPppAddrFilterReleases)

> PPP Released Due to Admin Commands (cCdmaPppAdminReleases)

> PPP Released Due to LCP Term Reqs (cCdmaPppLcpTermReleases)

> PPP Released Due to PCF Registration Request (cCdmaPppDeregisterByPcfReleases)

> PPP Released Due to Session Lifetime Expires (cCdmaPppLifetimeExpiryReleases)

### Total PPP Connections Released (PDSN or MS) (CCdmaPppTotalReleases)

Number of active PPP connections released by either the packet data serving node (PDSN) or mobile node since system startup.

### PPP Connections Released by PDSN (cCdmaPppPdsnReleases)

Number of active PPP connection release requests initiated by the PDSN since system startup.

### PPP Connections Released by Mobile (cCdmaPppMobileReleases)

Number of active PPP connection release requests initiated by the mobile node since system startup.

### PPP Released Due to Ingress Addr Filtering (cCdmaPppAddrFilterReleases)

Number of PPP connection releases due to ingress address filtering since system startup.

### PPP Released Due to Admin Commands (cCdmaPppAdminReleases)

Number of PPP connections released due to administrative commands since system startup.

### PPP Released Due to LCP Term Reqs (cCdmaPppLcpTermReleases)

Number of PPP connections released due to Link Control Protocol (LCP) term REQ since system startup.

### PPP Released Due to PCF Registration Request (cCdmaPppDeregisterByPcfReleases)

Total number of PPP connections released as Packet Control Function (PCF) sends deregistration request since system was last restarted.

Note: This object is available for PDSN version 3.0 and later.

### PPP Released Due to Session Lifetime Expires (cCdmaPppLifetimeExpiryReleases)

Total number of PPP connections released as the session lifetime expires, since the system was last restarted.

Note: This object is available for PDSN version 3.0 and later.