# RS-232 Port Configuration Information

The CiscoView Configure window displays the following information for an RS-232 port:

Index

Type

Input Signals

Output Signals

Input Speed

Output Speed

Output Flow Control

# Index (rs232PortIndex)

Specifies a unique value for each port. If possible, index values should map directly to external connectors.

# Type (rs232PortType)

Specifies the hardware type.

# Input Signals (rs232PortInSigNumber)

Specifies the number of detectable input signals for the port.

# Output Signals (rs232PortOutSigNumber)

Specifies the number of output signals the port can assert.

# Input Speed (rs232PortInSpeed)

Specifies the port's input speed in bits per second.

# Output Speed (rs232PortOutSpeed)

Specifies the output speed of the port in bits per second.

# Output Flow Control

Specifies the type of flow control the port is using.