# SSG Network Group

The SSG Network Group category of the Configure dialog box displays the service selection gateway (SSG) network group details.

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG Network Group from the Category list.

The following information appears:

Network Group Name (cssgNetworkGrpName)

Network Address Type (cssgNetworkGrpNetIpType)

Network Address (cssgNetworkGrpNetIpAddr)

Network Mask Type (cssgNetworkGrpNetMaskType)

Network Mask (cssgNetworkGrpNetMask)

Network Group RowStatus (cssgNetworkGrpNetRowStatus)

### Network Group Name (cssgNetworkGrpName)

Name of the network group. A network group, which is a group of networks, is associated with a server group for traffic redirection. Packets to networks in the network group are directed to servers in the server group.

### Network Address Type (cssgNetworkGrpNetIpType)

Value that represents the type of IP address in the object cssgNetworkGrpNetIpAddr.

### Network Address (cssgNetworkGrpNetIpAddr)

IP address of a network in the network group.

### Network Mask Type (cssgNetworkGrpNetMaskType)

Value that represents the type of address stored in cssgNetworkGrpNetMask.

### Network Mask (cssgNetworkGrpNetMask)

Mask to be combined with the destination address before the destination address is compared to the value in cssgNetworkGrpNetIpAddr.

### Network Group RowStatus (cssgNetworkGrpNetRowStatus)

Status of the table entry.

Status can be used to create or delete conceptual rows in the table.

To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

To delete a row, set the object to destroy.