# Monitoring DS1 Total Statistics

The CiscoView Monitor Port window displays the following total statistical information for a DS1 port:

Erred Secs (dsx1TotalESs)

Severe Erred Secs (dsx1TotalSESs)

Severe Erred Framing Secs (dsx1TotalSEFSs)

Unavail Erred Secs (dsx1TotalUASs)

Ctroled Slip Secs (dsx1TotalCSSs)

Path Coding Violates (dsx1TotalPCVs)

Line Erred Secs (dsx1TotalLESs)

Bursty Erred Secs (dsx1TotalBESs)

Degraded Mins (dsx1TotalDMs)

Line Code Violates (dsx1TotalLCVs)

# Erred Secs (dsx1TotalESs)

Shows the number of seconds during which errors were recorded for a DS1 interface during the previous 24-hour interval.

# Severe Erred Secs (dsx1TotalSESs)

Shows the number of seconds during which severe errors were recorded for a DS1 interface during the previous 24-hour interval.

# Severe Erred Framing Secs (dsx1TotalSEFSs)

Shows the number of seconds during which severe framing errors were recorded for a DS1 interface during the previous 24-hour interval.

# Unavail Erred Secs (dsx1TotalUASs)

Shows the number of seconds during which the specified DS1 interface was unavailable during the previous 24-hour interval.

# Ctroled Slip Secs (dsx1TotalCSSs)

Shows the number of seconds during which controlled slips were recorded for a DS1 interface during the previous 24-hour interval.

# Path Coding Violates (dsx1TotalPCVs)

Shows the number of path coding violations recorded for a DS1 interface during the previous 24-hour interval.

# Line Erred Secs (dsx1TotalLESs)

Shows the number of seconds during which line errors were recorded for a DS1 interface during the previous 24-hour interval.

# Bursty Erred Secs (dsx1TotalBESs)

Shows the number of seconds during which bursty errors were recorded for a DS1 interface during the previous 24-hour interval.

# Degraded Mins (dsx1TotalDMs)

Shows the number of degraded minutes recorded for a DS1 interface during the previous 24-hour interval.

# Line Code Violates (dsx1TotalLCVs)

Shows the number of line code violations recorded for a DS1 interface during the previous 24-hour interval.